Data Fields
gap_le_pkt_size_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Supported data length size Indication. More...

`#include <ble_gapc.h>`

## Data Fields
uint16_t | max_tx_octets
uint16_t | max_tx_time
uint16_t | max_rx_octets
uint16_t | max_rx_time

## Detailed Description

Supported data length size Indication.

## Field Documentation

## ◆ max_rx_octets

uint16_t gap_le_pkt_size_ind_t::max_rx_octets

The maximum number of payload octets in RX.

## ◆ max_rx_time

uint16_t gap_le_pkt_size_ind_t::max_rx_time

The maximum time that the local Controller will take to RX.

## ◆ max_tx_octets

uint16_t gap_le_pkt_size_ind_t::max_tx_octets

The maximum number of payload octets in TX.

## ◆ max_tx_time

uint16_t gap_le_pkt_size_ind_t::max_tx_time

The maximum time that the local Controller will take to TX.

The documentation for this struct was generated from the following file:

- ble_gapc.h