Data Fields
gap_chnl_map_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Channel map structure. More...

`#include <ble_gapc.h>`

## Data Fields
uint8_t | map [GAP_CHNL_MAP_LEN]

## Detailed Description

Channel map structure.

## Field Documentation

## ◆ map

uint8_t gap_chnl_map_t::map[GAP_CHNL_MAP_LEN]

This parameter contains 37 1-bit fields. The nth bit (n is in the range of 0 to 36) contains the value for the link layer channel index n. Channel n is unused = 0, channel n is used = 1. The most significant bits are reserved for future use.

The documentation for this struct was generated from the following file:

- ble_gapc.h