Macros
GAP ADV CHANNEL (bitmask)
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Defines

## Macros
#define | GAP_ADV_CHANNEL_37 0x01
#define | GAP_ADV_CHANNEL_38 0x02
#define | GAP_ADV_CHANNEL_39 0x04
#define | GAP_ADV_CHANNEL_37_38_39 0x07

## Detailed Description

## Macro Definition Documentation

## ◆ GAP_ADV_CHANNEL_37

#define GAP_ADV_CHANNEL_37 0x01

Advertising Channel 37 (2402MHz).

## ◆ GAP_ADV_CHANNEL_37_38_39

#define GAP_ADV_CHANNEL_37_38_39 0x07

Advertising Channel 37, 38, 39.

## ◆ GAP_ADV_CHANNEL_38

#define GAP_ADV_CHANNEL_38 0x02

Advertising Channel 38 (2426MHz).

## ◆ GAP_ADV_CHANNEL_39

#define GAP_ADV_CHANNEL_39 0x04

Advertising Channel 39 (2480MHz).