Data Fields
uds_regi_user_data_stream_t Struct Reference
BLE Services » User Data Service (UDS) » Structures

UDS Registered User Data stream. More...

`#include <uds.h>`

## Data Fields
uint8_t * | p_data
uint16_t | length
uint16_t | offset
uint16_t * | p_segm_length
uint16_t | segm_num
uint16_t | segm_offset

## Detailed Description

UDS Registered User Data stream.

## Field Documentation

## ◆ length

uint16_t uds_regi_user_data_stream_t::length

Length of Registered User Data stream.

## ◆ offset

uint16_t uds_regi_user_data_stream_t::offset

Offset of Registered User Data stream.

## ◆ p_data

uint8_t* uds_regi_user_data_stream_t::p_data

Pointer to Registered User Data stream.

## ◆ p_segm_length

uint16_t* uds_regi_user_data_stream_t::p_segm_length

Pointer to each segmentation length of Registered User Data stream.

## ◆ segm_num

uint16_t uds_regi_user_data_stream_t::segm_num

Registered User Data segmentations' number.

## ◆ segm_offset

uint16_t uds_regi_user_data_stream_t::segm_offset

Offset of Registered User Data segmentations' number.

The documentation for this struct was generated from the following file:

- uds.h