Macros
Test Mode
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SSI_NORMAL_MODE 0x00000000UL
#define | LL_SSI_TEST_MODE (1UL << SSI_CTRL0_SRL_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SSI_NORMAL_MODE

#define LL_SSI_NORMAL_MODE 0x00000000UL

Normal mode for SPI transfer

## ◆ LL_SSI_TEST_MODE

#define LL_SSI_TEST_MODE (1UL << SSI_CTRL0_SRL_Pos)

Test mode for SPI transfer: Rx and Tx connected inside