Data Fields
gap_dev_adv_tx_power_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

TX power info struct. More...

`#include <ble_gapc.h>`

## Data Fields
int8_t | power_lvl

## Detailed Description

TX power info struct.

## Field Documentation

## ◆ power_lvl

int8_t gap_dev_adv_tx_power_t::power_lvl

Advertising channel TX power level. Range: -20 to 10. Unit: dBm. Accuracy: +/-4dB.

The documentation for this struct was generated from the following file:

- ble_gapc.h