Data Fields
gap_peer_features_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

LE features info. More...

`#include <ble_gapc.h>`

## Data Fields
uint8_t | features [GAP_FEATS_LEN]

## Detailed Description

LE features info.

## Field Documentation

## ◆ features

uint8_t gap_peer_features_ind_t::features[GAP_FEATS_LEN]

8-byte array for LE features
Feature Setting field's bit mapping to Controller Features (0: not support, 1: support)

Bit position | Link Layer Feature
--- | ---
0 | LE Encryption
1 | Connection Parameters Request Procedure
2 | Extended Reject Indication
3 | Slave-initiated Features Exchange
4 | LE Ping
5 | LE Data Packet Length Extension
6 | LL Privacy
7 | Extended Scanner Filter Policies
8 | LE 2M PHY
9 | Stable Modulation Index - Transmitter
10 | Stable Modulation Index - Receiver
11 | LE Coded PHY
12 | LE Extended Advertising
13 | LE Periodic Advertising
14 | Channel Selection Algorithm #2
15 | LE Power Class 1
16 | Minimum Number of Used Channels Procedure
All other values | Reserved for Future Use

The documentation for this struct was generated from the following file:

- ble_gapc.h