Data Fields
_pkc_montgomery_inversion Struct Reference
Peripheral Driver » HAL Driver » PKC » Structures » PKC expression input

PKC Montgomery Inversion expression input. More...

`#include <gr55xx_hal_pkc.h>`

## Data Fields
uint32_t * | p_A
uint32_t * | p_P
uint32_t | ConstP

## Detailed Description

PKC Montgomery Inversion expression input.

Note
  Result = A^(-1) * 2^(K) mod P

## Field Documentation

## ◆ ConstP

uint32_t _pkc_montgomery_inversion::ConstP

Montgomery multiplication constant for P, where ConstP = (-P[0])^(-1) mod 2^32

## ◆ p_A

uint32_t* _pkc_montgomery_inversion::p_A

Pointer to operand A

## ◆ p_P

uint32_t* _pkc_montgomery_inversion::p_P

Pointer to prime number P

The documentation for this struct was generated from the following file:

- gr55xx_hal_pkc.h