Data Fields
gatt_common_cb_fun_t Struct Reference
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Common » Structures

GATT common callback function description. More...

`#include <ble_gatt.h>`

## Data Fields
void(* | app_gatt_mtu_exchange_cb )(uint8_t conn_idx, uint8_t status, uint16_t mtu)
void(* | app_gatt_prf_register_cb )(uint8_t status, uint8_t prf_index)

## Detailed Description

GATT common callback function description.

## Field Documentation

## ◆ app_gatt_mtu_exchange_cb

void(* gatt_common_cb_fun_t::app_gatt_mtu_exchange_cb) (uint8_t conn_idx, uint8_t status, uint16_t mtu)

Exchange MTU callback function.

## ◆ app_gatt_prf_register_cb

void(* gatt_common_cb_fun_t::app_gatt_prf_register_cb) (uint8_t status, uint8_t prf_index)

Profile register callback function.

Note
  prf_index range is from 0 to profile count - 1. prf_index is current profile index.

The documentation for this struct was generated from the following file:

- ble_gatt.h