Modules | Macros
Defines
BLE Services » Goodix UART Service Client (GUS_C)

## Modules
| Service and Characteristics UUID

## Macros
#define | GUS_C_CONNECTION_MAX
#define | FLOW_ON 0x01
#define | FLOW_OFF 0x00

## Detailed Description

## Macro Definition Documentation

## ◆ FLOW_OFF

#define FLOW_OFF 0x00

Indicate that GUS Client can not receive data from peer.

## ◆ FLOW_ON

#define FLOW_ON 0x01

Indicate that GUS Client can receive data from peer.

## ◆ GUS_C_CONNECTION_MAX

#define GUS_C_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of GUS Client connections.