Data Fields
cts_cur_time_t Struct Reference
BLE Services » Current Time Service (CTS) » Structures

CTS Current Time value. More...

`#include <cts.h>`

## Data Fields
cts_exact_time_256_t | day_date_time
uint8_t | adjust_reason

## Detailed Description

CTS Current Time value.

## Field Documentation

## ◆ adjust_reason

uint8_t cts_cur_time_t::adjust_reason

Adjust Reason.

## ◆ day_date_time

cts_exact_time_256_t cts_cur_time_t::day_date_time

Exact Time 256.

The documentation for this struct was generated from the following file:

- cts.h