Data Fields
sec_param_t Struct Reference
BLE » Security Manager(SM) » Structures

SEC Parameter. More...

`#include <ble_sec.h>`

## Data Fields
sec_mode_level_t | level
sec_io_cap_t | io_cap
bool | oob
uint8_t | auth
uint8_t | key_size
uint8_t | ikey_dist
uint8_t | rkey_dist

## Detailed Description

SEC Parameter.

## Field Documentation

## ◆ auth

uint8_t sec_param_t::auth

Set the auth, see SEC Auth Flag.

## ◆ ikey_dist

uint8_t sec_param_t::ikey_dist

Set the initial key distribution, see SEC Key Distribution Flag.

## ◆ io_cap

sec_io_cap_t sec_param_t::io_cap

Set the IO capability, see sec_io_cap_t.

## ◆ key_size

uint8_t sec_param_t::key_size

Indicate the supported maximum LTK size (range: 7-16).

## ◆ level

sec_mode_level_t sec_param_t::level

Set the minimum security level of the device, see sec_mode_level_t.

## ◆ oob

bool sec_param_t::oob

Indicate whether OOB is supported.

## ◆ rkey_dist

uint8_t sec_param_t::rkey_dist

Set the response key distribution, see SEC Key Distribution Flag.

The documentation for this struct was generated from the following file:

- ble_sec.h