Data Fields
gap_addr_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

The struct of address. More...

`#include <ble_gapc.h>`

## Data Fields
uint8_t | addr [GAP_ADDR_LEN]

## Detailed Description

The struct of address.

## Field Documentation

## ◆ addr

uint8_t gap_addr_t::addr[GAP_ADDR_LEN]

6-byte array address value.

The documentation for this struct was generated from the following file:

- ble_gapc.h