Data Fields
app_gpiote_param_t Struct Reference
Peripheral Driver » APP DRIVER » GPIO INTERRUPT » Structures

GPIOTE Interrupt parameters structure definition. More...

`#include <app_gpiote.h>`

## Data Fields
app_io_type_t | type
uint32_t | pin
app_io_mode_t | mode
app_io_pull_t | pull
app_handle_mode_t | handle_mode
app_io_callback_t | io_evt_cb

## Detailed Description

GPIOTE Interrupt parameters structure definition.

## Field Documentation

## ◆ handle_mode

app_handle_mode_t app_gpiote_param_t::handle_mode

Specifies the IO wakeup mode.

## ◆ io_evt_cb

app_io_callback_t app_gpiote_param_t::io_evt_cb

IO callback function.

## ◆ mode

app_io_mode_t app_gpiote_param_t::mode

Specifies the IO mode for the selected pins.

## ◆ pin

uint32_t app_gpiote_param_t::pin

Specifies the IO pins to be configured.

## ◆ pull

app_io_pull_t app_gpiote_param_t::pull

Specifies the Pull-up or Pull-Down activation for the selected pins.

## ◆ type

app_io_type_t app_gpiote_param_t::type

Specifies IO type

The documentation for this struct was generated from the following file:

- app_gpiote.h