Data Fields
gap_bdaddr_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

The struct of broadcast address with broadcast type. More...

`#include <ble_gapc.h>`

## Data Fields
gap_addr_t | gap_addr
uint8_t | addr_type

## Detailed Description

The struct of broadcast address with broadcast type.

## Field Documentation

## ◆ addr_type

uint8_t gap_bdaddr_t::addr_type

Address type of the device: 0=public/1=random. please GAP Address types.

## ◆ gap_addr

gap_addr_t gap_bdaddr_t::gap_addr

Device BD Address.

The documentation for this struct was generated from the following file:

- ble_gapc.h