Macros
Transfer Speed Mode
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants

## Macros
#define | LL_I2C_SPEED_MODE_STANDARD I2C_CON_SPEED_STANDARD
#define | LL_I2C_SPEED_MODE_FAST I2C_CON_SPEED_FAST
#define | LL_I2C_SPEED_MODE_HIGH I2C_CON_SPEED_HIGH

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_SPEED_MODE_FAST

#define LL_I2C_SPEED_MODE_FAST I2C_CON_SPEED_FAST

Fast (鈮?400 Kb/s) or Fast Plus mode (鈮?1000 螝b/s) of operation.

## ◆ LL_I2C_SPEED_MODE_HIGH

#define LL_I2C_SPEED_MODE_HIGH I2C_CON_SPEED_HIGH

High Speed mode (鈮?3.4 Mb/s) of operation.

## ◆ LL_I2C_SPEED_MODE_STANDARD

#define LL_I2C_SPEED_MODE_STANDARD I2C_CON_SPEED_STANDARD

Standard Speed mode(0 to 100 Kb/s) of operation.