Data Structures | Macros | Typedefs | Enumerations | Functions
gr55xx_hal_msio.h File Reference

Header file containing functions prototypes of MSIO HAL library. More...

`#include "gr55xx_ll_msio.h"`
`#include "gr55xx_hal_def.h"`
`#include "gr55xx_hal_msio_ex.h"`

Go to the source code of this file.

## Data Structures
struct | _msio_init
| MSIO init structure definition. More...

## Macros
#define | MSIO_PIN_0 ((uint16_t)0x0001U)
#define | MSIO_PIN_1 ((uint16_t)0x0002U)
#define | MSIO_PIN_2 ((uint16_t)0x0004U)
#define | MSIO_PIN_3 ((uint16_t)0x0008U)
#define | MSIO_PIN_4 ((uint16_t)0x0010U)
#define | MSIO_PIN_ALL ((uint16_t)0x001FU)
#define | MSIO_PIN_MASK (0x0000001FU)
#define | MSIO_DIRECTION_NONE LL_MSIO_DIRECTION_NONE
#define | MSIO_DIRECTION_INPUT LL_MSIO_DIRECTION_INPUT
#define | MSIO_DIRECTION_OUTPUT LL_MSIO_DIRECTION_OUTPUT
#define | MSIO_DIRECTION_INOUT LL_MSIO_DIRECTION_INOUT
#define | MSIO_MODE_ANALOG LL_MSIO_MODE_ANALOG
#define | MSIO_MODE_DIGITAL LL_MSIO_MODE_DIGITAL
#define | MSIO_NOPULL LL_MSIO_PULL_NO
#define | MSIO_PULLUP LL_MSIO_PULL_UP
#define | MSIO_PULLDOWN LL_MSIO_PULL_DOWN
#define | MSIO_DEFAULT_CONFIG
| MSIO_default_config initStruct default configuartion. More...
#define | IS_MSIO_PIN_ACTION(__ACTION__) (((__ACTION__) == MSIO_PIN_RESET) || ((__ACTION__) == MSIO_PIN_SET))
| Check if MSIO pin action is valid. More...
#define | IS_MSIO_PIN(__PIN__)
| Check if MSIO pins are valid. More...
#define | IS_MSIO_DIRECTION(__DIR__)
| Check if MSIO direction is valid. More...
#define | IS_MSIO_MODE(__MODE__)
| Check if MSIO mode is valid. More...
#define | IS_MSIO_PULL(__PULL__)
| Check if MSIO pull type is valid. More...

## Typedefs
typedef struct _msio_init | msio_init_t
| MSIO init structure definition.

## Enumerations
enum | msio_pin_state_t { MSIO_PIN_RESET = 0U, MSIO_PIN_SET }
| MSIO Bit SET and Bit RESET enumerations. More...

## Functions
void | hal_msio_init (msio_init_t *p_msio_init)
| Initialize the MSIOx peripheral according to the specified parameters in the msio_init_t. More...
void | hal_msio_deinit (uint32_t msio_pin)
| De-initialize the MSIOx peripheral registers to their default reset values. More...
msio_pin_state_t | hal_msio_read_pin (uint16_t msio_pin)
| Read the specified input port pin. More...
void | hal_msio_write_pin (uint16_t msio_pin, msio_pin_state_t pin_state)
| Set or clear the selected data port bit. More...
void | hal_msio_toggle_pin (uint16_t msio_pin)
| Toggle the specified MSIO pin. More...

## Detailed Description

Header file containing functions prototypes of MSIO HAL library.

Author
  BLE Driver Team

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.