Data Fields
lecb_conn_ind_t Struct Reference
BLE » Logical Link Control and Adaptation Protocol (L2CAP) » Structures

LE credit based connection created indication. More...

`#include <ble_l2cap.h>`

## Data Fields
uint16_t | le_psm
uint16_t | local_cid
uint16_t | local_credits
uint16_t | peer_credits
uint16_t | peer_mtu
uint16_t | peer_mps

## Detailed Description

LE credit based connection created indication.

## Field Documentation

## ◆ le_psm

uint16_t lecb_conn_ind_t::le_psm

Le_psm number.

## ◆ local_cid

uint16_t lecb_conn_ind_t::local_cid

The local source channel ID.

## ◆ local_credits

uint16_t lecb_conn_ind_t::local_credits

It indicates the number of LE-frames that the local device can receive.

## ◆ peer_credits

uint16_t lecb_conn_ind_t::peer_credits

It indicates the number of LE-frames that the peer device can receive.

## ◆ peer_mps

uint16_t lecb_conn_ind_t::peer_mps

It indicates the maximum payload size (in octets) that the L2CAP layer entity sending the LE Credit Based Connection Request is capable of receiving on this channe.

## ◆ peer_mtu

uint16_t lecb_conn_ind_t::peer_mtu

It indicates the maximum SDU size (in octets) that the L2CAP layer entity sending the LE Credit Based Connection Request can receive on this channel.

The documentation for this struct was generated from the following file:

- ble_l2cap.h