Data Fields
rscs_meas_val_t Struct Reference
BLE Services » Running Speed and Cadence Service (RSCS) » Structures

Running Speed and Cadence Measurement Character value structure. More...

`#include <rscs.h>`

## Data Fields
bool | inst_stride_length_present
bool | total_distance_present
bool | is_run_or_walk
uint16_t | inst_speed
uint8_t | inst_cadence
uint16_t | inst_stride_length
uint32_t | total_distance

## Detailed Description

Running Speed and Cadence Measurement Character value structure.

## Field Documentation

## ◆ inst_cadence

uint8_t rscs_meas_val_t::inst_cadence

Instantaneous Cadence.

## ◆ inst_speed

uint16_t rscs_meas_val_t::inst_speed

Instantaneous Speed.

## ◆ inst_stride_length

uint16_t rscs_meas_val_t::inst_stride_length

Instantaneous Stride Length.

## ◆ inst_stride_length_present

bool rscs_meas_val_t::inst_stride_length_present

If Instantaneous Stride Length is present.

## ◆ is_run_or_walk

bool rscs_meas_val_t::is_run_or_walk

True: Running, False: Walking.

## ◆ total_distance

uint32_t rscs_meas_val_t::total_distance

Total Distance.

## ◆ total_distance_present

bool rscs_meas_val_t::total_distance_present

If Total Distance is present.

The documentation for this struct was generated from the following file:

- rscs.h