Data Fields
gap_le_phy_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

PHY info. More...

`#include <ble_gapc.h>`

## Data Fields
uint8_t | tx_phy
uint8_t | rx_phy

## Detailed Description

PHY info.

## Field Documentation

## ◆ rx_phy

uint8_t gap_le_phy_ind_t::rx_phy

LE PHY for data reception.

See also
  GAP PHYs (bitmask).

## ◆ tx_phy

uint8_t gap_le_phy_ind_t::tx_phy

LE PHY for data transmission.

See also
  GAP PHYs (bitmask).

The documentation for this struct was generated from the following file:

- ble_gapc.h