Data Fields
gap_max_adv_data_len_ind_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control » Structures

Maximum advertising data length info. More...

`#include <ble_gapc.h>`

## Data Fields
uint16_t | length

## Detailed Description

Maximum advertising data length info.

## Field Documentation

## ◆ length

uint16_t gap_max_adv_data_len_ind_t::length

Maximum advertising data length supported by controller.

The documentation for this struct was generated from the following file:

- ble_gapc.h