Data Structures | Macros | Typedefs | Enumerations | Functions
dis_c.h File Reference

Device Information Service Client API. More...

`#include "gr55xx_sys.h"`
`#include "ble_prf_types.h"`
`#include "custom_config.h"`
`#include <stdint.h>`
`#include <stdbool.h>`

Go to the source code of this file.

## Data Structures
struct | dis_c_handles_t
| Handles on the connected peer device needed to interact with it. More...
struct | dis_c_string_t
| Response data for string-based DIS characteristics. More...
struct | dis_c_sys_id_t
| Response data for System ID parameters. More...
struct | dis_c_reg_cert_data_list_t
| Response data for IEEE 11073-20601 Regulatory Certification Data List Structure. More...
struct | dis_c_pnp_id_t
| Response data for PnP ID parameters. More...
struct | ble_dis_c_read_rsp_t
| Device Information Service Client Read Response encode structure. More...
struct | dis_c_evt_t
| Device Information Service Client event. More...

## Macros
#define | DIS_C_CONNECTION_MAX
#define | DIS_C_STRING_LEN_MAX 128
#define | DIS_C_11073_BODY_EMPTY 0
#define | DIS_C_11073_BODY_IEEE 1
#define | DIS_C_11073_BODY_CONTINUA 2
#define | DIS_C_11073_BODY_EXP 254

## Typedefs
typedef void(* | dis_c_evt_handler_t) (dis_c_evt_t *p_evt)
| Device Information Service Client event handler type.

## Enumerations
enum | dis_c_evt_type_t { DIS_C_EVT_INVALID, DIS_C_EVT_DISCOVERY_COMPLETE, DIS_C_EVT_DISCOVERY_FAIL, DIS_C_EVT_DEV_INFORMATION_READ_RSP }
| Device Information Service Client event type. More...
enum | dis_c_char_type_t { DIS_C_SYS_ID, DIS_C_MODEL_NUM, DIS_C_SERIAL_NUM, DIS_C_HW_REV, DIS_C_FW_REV, DIS_C_SW_REV, DIS_C_MANUF_NAME, DIS_C_CERT_LIST, DIS_C_PNP_ID, DIS_C_CHARACTER_NB }
| Device Information Service Client characteristic type. More...

## Functions
sdk_err_t | dis_client_init (dis_c_evt_handler_t evt_handler)
| Register DIS Client event handler. More...
sdk_err_t | dis_c_disc_srvc_start (uint8_t conn_idx)
| Discovery Device Information Service on peer. More...
sdk_err_t | dis_c_char_value_read (uint8_t conn_idx, dis_c_char_type_t char_read_type)
| Read Device Information Service characteristic value. More...

## Detailed Description

Device Information Service Client API.