Data Fields
_ll_aes_init Struct Reference
Peripheral Driver » LL Driver » AES » Structures » AES Exported Init structures

LL AES Init Structure definition. More...

`#include <gr55xx_ll_aes.h>`

## Data Fields
uint32_t | key_size
uint32_t * | p_key
uint32_t * | p_init_vector
uint32_t * | p_seed

## Detailed Description

LL AES Init Structure definition.

## Field Documentation

## ◆ key_size

uint32_t _ll_aes_init::key_size

128, 192 or 256-bit key length. This parameter can be a value of Key Size

## ◆ p_init_vector

uint32_t* _ll_aes_init::p_init_vector

Initialization Vector used for CBC modes

## ◆ p_key

uint32_t* _ll_aes_init::p_key

Encryption/Decryption Key

## ◆ p_seed

uint32_t* _ll_aes_init::p_seed

Random seeds

The documentation for this struct was generated from the following file:

- gr55xx_ll_aes.h