### - t -

- temp_convert_value : hts_meas_val_t
- temp_meas_type : hts_meas_val_t
- temp_original_value : hts_meas_val_t
- temp_type : hts_init_t , hts_meas_val_t
- temperature_units : hts_init_t
- tester_and_health : gls_meas_ctx_t
- ths_rx_handle : ths_c_handles_t
- ths_setting_cccd_handle : ths_c_handles_t
- ths_setting_handle : ths_c_handles_t
- ths_srvc_end_handle : ths_c_handles_t
- ths_srvc_start_handle : ths_c_handles_t
- ths_toggle_handle : ths_c_handles_t
- ths_tx_cccd_handle : ths_c_handles_t
- ths_tx_handle : ths_c_handles_t
- ti_mode : _spi_init
- time : gls_racp_filter_t
- time_init : _calendar_handle
- time_offset : gls_meas_val_t
- time_stamp : bcs_meas_val_t , bps_meas_t , hts_meas_val_t
- time_stamp_present : bcs_meas_flag_t , bps_meas_t , hts_init_t
- time_zone : cts_c_loc_time_info_t , cts_loc_time_info_t
- timeout : _aes_handle , _hmac_handle , _i2s_handle , _pkc_handle , _qspi_handle , _spi_handle , gap_scan_param_t
- timer_msp_deinit : _hal_timer_callback
- timer_msp_init : _hal_timer_callback
- timer_period_elapsed_callback : _hal_timer_callback
- tk : sec_cfm_enc_data_t
- tk_type : sec_enc_req_data_t
- total_distance : rscs_c_meas_val_t , rscs_meas_val_t
- total_distance_present : rscs_c_meas_val_t , rscs_meas_val_t
- tps_srvc_end_handle : tps_c_handles_t
- tps_srvc_start_handle : tps_c_handles_t
- tps_tx_power_level_handle : tps_c_handles_t
- transfer_direction : _ll_qspi_init_t , _ll_spim_init_t
- transport_mode : ths_init_t
- trigger : _ll_aon_gpio_init , _ll_gpio_init
- twext : ble_slp_config_t
- twosc : ble_slp_config_t
- twrm : ble_slp_config_t
- tx : app_uart_pin_cfg_t
- tx_buf : app_uart_tx_buf_t
- tx_buf_size : app_uart_tx_buf_t
- tx_dma_channel : app_i2c_mode_t , app_i2s_mode_t , app_spi_mode_t , app_uart_mode_t
- tx_path_comp : gap_dev_rf_path_comp_ind_t
- tx_phy : gap_le_phy_ind_t
- tx_power : rf_trim_info_t
- tx_power_level : tps_c_evt_t
- tx_pwr : gap_ext_adv_report_ind_t
- tx_state : _iso7816_handle_t , _uart_handle
- tx_threshold : _ll_i2s_init_t
- tx_xfer_count : _i2s_handle , _iso7816_handle_t , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- tx_xfer_size : _i2s_handle , _iso7816_handle_t , _qspi_handle , _spi_handle , _uart_handle , _xqspi_handle_t
- txdata_size : _ll_i2s_init_t
- txpwr_dbm : gdx_lcp_config_t
- type : app_adc_evt_t , app_adc_mode_t , app_adc_pin_t , app_aes_evt_t , app_comp_pin_t , app_gpiote_evt_t , app_gpiote_param_t , app_hmac_evt_t , app_i2c_evt_t , app_i2c_mode_t , app_i2c_pin_t , app_i2s_evt_t , app_i2s_mode_t , app_i2s_pin_t , app_pkc_evt_t , app_pwm_pin_t , app_qspi_evt_t , app_qspi_mode_t , app_qspi_pin_t , app_rng_evt_t , app_rtc_evt_t , app_spi_evt_t , app_spi_mode_t , app_spi_pin_t , app_uart_evt_t , app_uart_mode_t , app_uart_pin_t , ble_gattc_ntf_ind_t , ble_gatts_ntf_ind_t , gap_ext_adv_param_t , gap_ext_init_param_t , gap_ext_scan_param_t , gap_init_param_t , gap_per_sync_param_t , gatts_noti_ind_t , gls_meas_val_t