Macros
DMA Peripheral type
Peripheral Driver » LL Driver » DMA » Defines » DMA Exported Constants

## Macros
#define | LL_DMA_PERIPH_SPIM_TX ((uint32_t)0x00000000U)
#define | LL_DMA_PERIPH_SPIM_RX ((uint32_t)0x00000001U)
#define | LL_DMA_PERIPH_SPIS_TX ((uint32_t)0x00000002U)
#define | LL_DMA_PERIPH_SPIS_RX ((uint32_t)0x00000003U)
#define | LL_DMA_PERIPH_QSPI0_TX ((uint32_t)0x00000004U)
#define | LL_DMA_PERIPH_QSPI0_RX ((uint32_t)0x00000005U)
#define | LL_DMA_PERIPH_I2C0_TX ((uint32_t)0x00000006U)
#define | LL_DMA_PERIPH_I2C0_RX ((uint32_t)0x00000007U)
#define | LL_DMA_PERIPH_I2C1_TX ((uint32_t)0x00000008U)
#define | LL_DMA_PERIPH_I2C1_RX ((uint32_t)0x00000009U)
#define | LL_DMA_PERIPH_I2S_S_TX ((uint32_t)0x00000008U)
#define | LL_DMA_PERIPH_I2S_S_RX ((uint32_t)0x00000009U)
#define | LL_DMA_PERIPH_UART0_TX ((uint32_t)0x0000000AU)
#define | LL_DMA_PERIPH_UART0_RX ((uint32_t)0x0000000BU)
#define | LL_DMA_PERIPH_QSPI1_TX ((uint32_t)0x0000000CU)
#define | LL_DMA_PERIPH_QSPI1_RX ((uint32_t)0x0000000DU)
#define | LL_DMA_PERIPH_I2S_M_TX ((uint32_t)0x0000000CU)
#define | LL_DMA_PERIPH_I2S_M_RX ((uint32_t)0x0000000DU)
#define | LL_DMA_PERIPH_SNSADC ((uint32_t)0x0000000EU)
#define | LL_DMA_PERIPH_MEM ((uint32_t)0x0000000FU)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_DMA_PERIPH_I2C0_RX

#define LL_DMA_PERIPH_I2C0_RX ((uint32_t)0x00000007U)

DMA Peripheral type is I2C0 RX

## ◆ LL_DMA_PERIPH_I2C0_TX

#define LL_DMA_PERIPH_I2C0_TX ((uint32_t)0x00000006U)

DMA Peripheral type is I2C0 TX

## ◆ LL_DMA_PERIPH_I2C1_RX

#define LL_DMA_PERIPH_I2C1_RX ((uint32_t)0x00000009U)

DMA Peripheral type is I2C1 RX

## ◆ LL_DMA_PERIPH_I2C1_TX

#define LL_DMA_PERIPH_I2C1_TX ((uint32_t)0x00000008U)

DMA Peripheral type is I2C1 TX

## ◆ LL_DMA_PERIPH_I2S_M_RX

#define LL_DMA_PERIPH_I2S_M_RX ((uint32_t)0x0000000DU)

DMA Peripheral type is I2S_M RX

## ◆ LL_DMA_PERIPH_I2S_M_TX

#define LL_DMA_PERIPH_I2S_M_TX ((uint32_t)0x0000000CU)

DMA Peripheral type is I2S_M TX

## ◆ LL_DMA_PERIPH_I2S_S_RX

#define LL_DMA_PERIPH_I2S_S_RX ((uint32_t)0x00000009U)

DMA Peripheral type is I2S_S RX

## ◆ LL_DMA_PERIPH_I2S_S_TX

#define LL_DMA_PERIPH_I2S_S_TX ((uint32_t)0x00000008U)

DMA Peripheral type is I2S_S TX

## ◆ LL_DMA_PERIPH_MEM

#define LL_DMA_PERIPH_MEM ((uint32_t)0x0000000FU)

DMA peripheral type is Memory

## ◆ LL_DMA_PERIPH_QSPI0_RX

#define LL_DMA_PERIPH_QSPI0_RX ((uint32_t)0x00000005U)

DMA Peripheral type is QSPI0 RX

## ◆ LL_DMA_PERIPH_QSPI0_TX

#define LL_DMA_PERIPH_QSPI0_TX ((uint32_t)0x00000004U)

DMA Peripheral type is QSPI0 TX

## ◆ LL_DMA_PERIPH_QSPI1_RX

#define LL_DMA_PERIPH_QSPI1_RX ((uint32_t)0x0000000DU)

DMA peripheral type is QSPI1 RX

## ◆ LL_DMA_PERIPH_QSPI1_TX

#define LL_DMA_PERIPH_QSPI1_TX ((uint32_t)0x0000000CU)

DMA peripheral type is QSPI1 TX

## ◆ LL_DMA_PERIPH_SNSADC

#define LL_DMA_PERIPH_SNSADC ((uint32_t)0x0000000EU)

DMA peripheral type is SNSADC

## ◆ LL_DMA_PERIPH_SPIM_RX

#define LL_DMA_PERIPH_SPIM_RX ((uint32_t)0x00000001U)

DMA Peripheral type is SPIM RX

## ◆ LL_DMA_PERIPH_SPIM_TX

#define LL_DMA_PERIPH_SPIM_TX ((uint32_t)0x00000000U)

DMA Peripheral type is SPIM TX

## ◆ LL_DMA_PERIPH_SPIS_RX

#define LL_DMA_PERIPH_SPIS_RX ((uint32_t)0x00000003U)

DMA Peripheral type is SPIS RX

## ◆ LL_DMA_PERIPH_SPIS_TX

#define LL_DMA_PERIPH_SPIS_TX ((uint32_t)0x00000002U)

DMA Peripheral type is SPIS TX

## ◆ LL_DMA_PERIPH_UART0_RX

#define LL_DMA_PERIPH_UART0_RX ((uint32_t)0x0000000BU)

DMA Peripheral type is UART0 RX

## ◆ LL_DMA_PERIPH_UART0_TX

#define LL_DMA_PERIPH_UART0_TX ((uint32_t)0x0000000AU)

DMA Peripheral type is UART0 TX