Macros
XQSPI Instruction and Address Mode, only in QSPI mode
Peripheral Driver » HAL Driver » XQSPI » Defines » XQSPI Exported Constants

## Macros
#define | XQSPI_INST_ADDR_ALL_IN_SPI (0)
#define | XQSPI_INST_IN_SPI_ADDR_IN_SPIFRF (1)
#define | XQSPI_INST_ADDR_ALL_IN_SPIFRF (2)

## Detailed Description

## Macro Definition Documentation

## ◆ XQSPI_INST_ADDR_ALL_IN_SPI

#define XQSPI_INST_ADDR_ALL_IN_SPI (0)

Instruction and address are sent in SPI mode

## ◆ XQSPI_INST_ADDR_ALL_IN_SPIFRF

#define XQSPI_INST_ADDR_ALL_IN_SPIFRF (2)

Instruction and address are sent in Daul/Quad SPI mode

## ◆ XQSPI_INST_IN_SPI_ADDR_IN_SPIFRF

#define XQSPI_INST_IN_SPI_ADDR_IN_SPIFRF (1)

Instruction is sent in SPI mode, and address is sent in Daul/Quad SPI mode