Data Fields
_ll_spis_init_t Struct Reference
Peripheral Driver » LL Driver » SPI » Structures » SPI Exported init structure

SPIS init structures definition. More...

`#include <gr55xx_ll_spi.h>`

## Data Fields
uint32_t | data_size
uint32_t | clock_polarity
uint32_t | clock_phase

## Detailed Description

SPIS init structures definition.

## Field Documentation

## ◆ clock_phase

uint32_t _ll_spis_init_t::clock_phase

Specifies the clock active edge for the bit capture. This parameter can be a value of Clock Phase.

This feature can be modified afterwards using unitary function ll_spi_set_clock_phase().

## ◆ clock_polarity

uint32_t _ll_spis_init_t::clock_polarity

Specifies the serial clock steady state. This parameter can be a value of Clock Polarity.

This feature can be modified afterwards using unitary function ll_spi_set_clock_polarity().

## ◆ data_size

uint32_t _ll_spis_init_t::data_size

Specifies the SPI data width. This parameter can be a value of Datawidth.

This feature can be modified afterwards using unitary function ll_spi_set_data_size().

The documentation for this struct was generated from the following file:

- gr55xx_ll_spi.h