### - l -

- LL_ADC_CLK_1 : gr55xx_ll_adc.h
- LL_ADC_CLK_16 : gr55xx_ll_adc.h
- LL_ADC_CLK_1P6 : gr55xx_ll_adc.h
- LL_ADC_CLK_2 : gr55xx_ll_adc.h
- LL_ADC_CLK_4 : gr55xx_ll_adc.h
- LL_ADC_CLK_8 : gr55xx_ll_adc.h
- LL_ADC_DEFAULT_CONFIG : gr55xx_ll_adc.h
- LL_ADC_INPUT_DIFFERENTIAL : gr55xx_ll_adc.h
- LL_ADC_INPUT_SINGLE : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_BAT : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO0 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO1 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO2 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO3 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_IO4 : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_REF : gr55xx_ll_adc.h
- LL_ADC_INPUT_SRC_TMP : gr55xx_ll_adc.h
- LL_ADC_ReadReg : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_BUF_INT : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_IO0 : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_IO1 : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_IO2 : gr55xx_ll_adc.h
- LL_ADC_REF_SRC_IO3 : gr55xx_ll_adc.h
- LL_ADC_REF_VALUE_0P8 : gr55xx_ll_adc.h
- LL_ADC_REF_VALUE_1P2 : gr55xx_ll_adc.h
- LL_ADC_REF_VALUE_1P6 : gr55xx_ll_adc.h
- LL_ADC_WriteReg : gr55xx_ll_adc.h
- LL_AES_DMA_TRANSIZE_MAX : gr55xx_ll_aes.h
- LL_AES_DMA_TRANSIZE_MIN : gr55xx_ll_aes.h
- LL_AES_FLAG_DATAREADY : gr55xx_ll_aes.h
- LL_AES_FLAG_DMA_DONE : gr55xx_ll_aes.h
- LL_AES_FLAG_DMA_ERR : gr55xx_ll_aes.h
- LL_AES_FLAG_KEY_VALID : gr55xx_ll_aes.h
- LL_AES_KEY_SIZE_128 : gr55xx_ll_aes.h
- LL_AES_KEY_SIZE_192 : gr55xx_ll_aes.h
- LL_AES_KEY_SIZE_256 : gr55xx_ll_aes.h
- LL_AES_KEYTYPE_AHB : gr55xx_ll_aes.h
- LL_AES_KEYTYPE_KRAM : gr55xx_ll_aes.h
- LL_AES_KEYTYPE_MCU : gr55xx_ll_aes.h
- LL_AES_OPERATION_MODE_CBC : gr55xx_ll_aes.h
- LL_AES_OPERATION_MODE_ECB : gr55xx_ll_aes.h
- LL_AES_ReadReg : gr55xx_ll_aes.h
- LL_AES_WriteReg : gr55xx_ll_aes.h
- LL_AON_GPIO_DEFAULT_CONFIG : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MODE_INPUT : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MODE_MUX : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MODE_OUTPUT : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_0 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_1 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_2 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_3 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_4 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_5 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_6 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_7 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_MUX_8 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_0 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_1 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_2 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_3 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_4 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_5 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_6 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_7 : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PIN_ALL : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PULL_DOWN : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PULL_NO : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_PULL_UP : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RE_N : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RE_N_Msk : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RE_N_Pos : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_ReadReg : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RTYP : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RTYP_Msk : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_RTYP_Pos : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_FALLING : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_HIGH : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_LOW : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_NONE : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_TRIGGER_RISING : gr55xx_ll_aon_gpio.h
- LL_AON_GPIO_WriteReg : gr55xx_ll_aon_gpio.h
- LL_CALENDAR_DIV_128 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_256 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_32 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_64 : gr55xx_ll_calendar.h
- LL_CALENDAR_DIV_NONE : gr55xx_ll_calendar.h
- LL_CALENDAR_NO_CLOCK : gr55xx_ll_calendar.h
- LL_CGC_DEFAULT_CONFIG : gr55xx_ll_cgc.h
- LL_CGC_FRC_ALL_HCLK0 : gr55xx_ll_cgc.h
- LL_CGC_FRC_ALL_HCLK1 : gr55xx_ll_cgc.h
- LL_CGC_FRC_ALL_HCLK2 : gr55xx_ll_cgc.h
- LL_CGC_FRC_AON_MCUSUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_APB_SUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_BLE_BRG_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_DMA_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_GPIO_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_HTB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2C0_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2C1_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2S_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_I2S_S_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_PWM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_QSPI0_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_QSPI1_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_ROM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SECU_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SECU_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SERIAL_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SERIALS_HCLK2 : gr55xx_ll_cgc.h
- LL_CGC_FRC_SIM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SNSADC_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SPIM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SPIS_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_SRAM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_UART0_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_UART1_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_XF_XQSPI_HCLK : gr55xx_ll_cgc.h
- LL_CGC_FRC_XQSPI_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_ReadReg : gr55xx_ll_cgc.h
- LL_CGC_WFI_ALL_HCLK0 : gr55xx_ll_cgc.h
- LL_CGC_WFI_ALL_HCLK1 : gr55xx_ll_cgc.h
- LL_CGC_WFI_ALL_HCLK2 : gr55xx_ll_cgc.h
- LL_CGC_WFI_AON_MCUSUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_APB_SUB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_BLE_BRG_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_DMA_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_GPIO_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_HTB_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_I2S_S_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_PWM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_ROM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SECU_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SECU_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SERIAL_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SIM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SNSADC_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_SRAM_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_XF_XQSPI_HCLK : gr55xx_ll_cgc.h
- LL_CGC_WFI_XQSPI_DIV4_PCLK : gr55xx_ll_cgc.h
- LL_CGC_WriteReg : gr55xx_ll_cgc.h
- LL_COMP_DEFAULT_CONFIG : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO0 : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO1 : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO2 : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO3 : gr55xx_ll_comp.h
- LL_COMP_INPUT_SRC_IO4 : gr55xx_ll_comp.h
- LL_COMP_ReadReg : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO0 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO1 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO2 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO3 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_IO4 : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_VBAT : gr55xx_ll_comp.h
- LL_COMP_REF_SRC_VREF : gr55xx_ll_comp.h
- LL_COMP_WriteReg : gr55xx_ll_comp.h
- LL_DMA_CHANNEL_0 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_1 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_2 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_3 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_4 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_5 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_6 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_7 : gr55xx_ll_dma.h
- LL_DMA_CHANNEL_ALL : gr55xx_ll_dma.h
- LL_DMA_DDATAALIGN_BYTE : gr55xx_ll_dma.h
- LL_DMA_DDATAALIGN_HALFWORD : gr55xx_ll_dma.h
- LL_DMA_DDATAALIGN_WORD : gr55xx_ll_dma.h
- LL_DMA_DHANDSHAKING_HW : gr55xx_ll_dma.h
- LL_DMA_DHANDSHAKING_SW : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_MEMORY_TO_MEMORY : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_MEMORY_TO_PERIPH : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_PERIPH_TO_MEMORY : gr55xx_ll_dma.h
- LL_DMA_DIRECTION_PERIPH_TO_PERIPH : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_1 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_16 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_32 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_4 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_64 : gr55xx_ll_dma.h
- LL_DMA_DST_BURST_LENGTH_8 : gr55xx_ll_dma.h
- LL_DMA_DST_DECREMENT : gr55xx_ll_dma.h
- LL_DMA_DST_INCREMENT : gr55xx_ll_dma.h
- LL_DMA_DST_NO_CHANGE : gr55xx_ll_dma.h
- LL_DMA_MODE_MULTI_BLOCK_ALL_RELOAD : gr55xx_ll_dma.h
- LL_DMA_MODE_MULTI_BLOCK_DST_RELOAD : gr55xx_ll_dma.h
- LL_DMA_MODE_MULTI_BLOCK_SRC_RELOAD : gr55xx_ll_dma.h
- LL_DMA_MODE_SINGLE_BLOCK : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2C0_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2C0_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2C1_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2C1_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2S_M_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2S_M_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2S_S_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_I2S_S_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_MEM : gr55xx_ll_dma.h
- LL_DMA_PERIPH_QSPI0_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_QSPI0_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_QSPI1_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_QSPI1_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SNSADC : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SPIM_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SPIM_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SPIS_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_SPIS_TX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_UART0_RX : gr55xx_ll_dma.h
- LL_DMA_PERIPH_UART0_TX : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_0 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_1 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_2 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_3 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_4 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_5 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_6 : gr55xx_ll_dma.h
- LL_DMA_PRIORITY_7 : gr55xx_ll_dma.h
- LL_DMA_ReadReg : gr55xx_ll_dma.h
- LL_DMA_SDATAALIGN_BYTE : gr55xx_ll_dma.h
- LL_DMA_SDATAALIGN_HALFWORD : gr55xx_ll_dma.h
- LL_DMA_SDATAALIGN_WORD : gr55xx_ll_dma.h
- LL_DMA_SHANDSHAKING_HW : gr55xx_ll_dma.h
- LL_DMA_SHANDSHAKING_SW : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_1 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_16 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_32 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_4 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_64 : gr55xx_ll_dma.h
- LL_DMA_SRC_BURST_LENGTH_8 : gr55xx_ll_dma.h
- LL_DMA_SRC_DECREMENT : gr55xx_ll_dma.h
- LL_DMA_SRC_INCREMENT : gr55xx_ll_dma.h
- LL_DMA_SRC_NO_CHANGE : gr55xx_ll_dma.h
- LL_DMA_WriteReg : gr55xx_ll_dma.h
- LL_DUAL_TIMER_COUNTERSIZE_16 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_COUNTERSIZE_32 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_FREERUNNING_MODE : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PERIODIC_MODE : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV0 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV16 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_PRESCALER_DIV256 : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_ReadReg : gr55xx_ll_dual_tim.h
- LL_DUAL_TIMER_WriteReg : gr55xx_ll_dual_tim.h
- LL_ECC_CURVE_DEFAULT_CONFIG : gr55xx_ll_pkc.h
- LL_EFUSE_CRC_CHECK : gr55xx_ll_efuse.h
- LL_EFUSE_CRC_CHECK_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_CRC_CHECK_SUCCESS : gr55xx_ll_efuse.h
- LL_EFUSE_INIT_CHECK : gr55xx_ll_efuse.h
- LL_EFUSE_INIT_CHECK_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_INIT_CHECK_SUCCESS : gr55xx_ll_efuse.h
- LL_EFUSE_PWR_CTL_DIS_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_PWR_CTL_EN_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_READ_TRIM : gr55xx_ll_efuse.h
- LL_EFUSE_READ_TRIM_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_ReadReg : gr55xx_ll_efuse.h
- LL_EFUSE_TEST_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_TEST_READ : gr55xx_ll_efuse.h
- LL_EFUSE_WRITE_DONE : gr55xx_ll_efuse.h
- LL_EFUSE_WRITE_KEYRAM : gr55xx_ll_efuse.h
- LL_EFUSE_WRITE_KEYRAM_BUSY : gr55xx_ll_efuse.h
- LL_EFUSE_WriteReg : gr55xx_ll_efuse.h
- LL_GPIO_DEFAULT_CONFIG : gr55xx_ll_gpio.h
- LL_GPIO_GET_REG_MUX_CTRL_0_7 : gr55xx_ll_gpio.h
- LL_GPIO_GET_REG_MUX_CTRL_8_15 : gr55xx_ll_gpio.h
- LL_GPIO_GET_RESISTOR_POS : gr55xx_ll_gpio.h
- LL_GPIO_MODE_INPUT : gr55xx_ll_gpio.h
- LL_GPIO_MODE_MUX : gr55xx_ll_gpio.h
- LL_GPIO_MODE_OUTPUT : gr55xx_ll_gpio.h
- LL_GPIO_MUX_0 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_1 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_2 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_3 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_4 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_5 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_6 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_7 : gr55xx_ll_gpio.h
- LL_GPIO_MUX_8 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_0 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_1 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_10 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_11 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_12 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_13 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_14 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_15 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_2 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_3 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_4 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_5 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_6 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_7 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_8 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_9 : gr55xx_ll_gpio.h
- LL_GPIO_PIN_ALL : gr55xx_ll_gpio.h
- LL_GPIO_PULL_DOWN : gr55xx_ll_gpio.h
- LL_GPIO_PULL_NO : gr55xx_ll_gpio.h
- LL_GPIO_PULL_UP : gr55xx_ll_gpio.h
- LL_GPIO_RE_N : gr55xx_ll_gpio.h
- LL_GPIO_RE_N_Msk : gr55xx_ll_gpio.h
- LL_GPIO_RE_N_Pos : gr55xx_ll_gpio.h
- LL_GPIO_ReadReg : gr55xx_ll_gpio.h
- LL_GPIO_RTYP : gr55xx_ll_gpio.h
- LL_GPIO_RTYP_Msk : gr55xx_ll_gpio.h
- LL_GPIO_RTYP_Pos : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_FALLING : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_HIGH : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_LOW : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_NONE : gr55xx_ll_gpio.h
- LL_GPIO_TRIGGER_RISING : gr55xx_ll_gpio.h
- LL_GPIO_WriteReg : gr55xx_ll_gpio.h
- LL_HMAC_CALCULATETYPE_HMAC : gr55xx_ll_hmac.h
- LL_HMAC_CALCULATETYPE_SHA : gr55xx_ll_hmac.h
- LL_HMAC_DMA_TRANSIZE_MAX : gr55xx_ll_hmac.h
- LL_HMAC_DMA_TRANSIZE_MIN : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DATAREADY_HMAC : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DATAREADY_SHA : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DMA_DONE : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DMA_ERR : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_DMA_MESSAGEDONE : gr55xx_ll_hmac.h
- LL_HMAC_FLAG_KEY_VALID : gr55xx_ll_hmac.h
- LL_HMAC_HASH_STANDARD : gr55xx_ll_hmac.h
- LL_HMAC_HASH_USER : gr55xx_ll_hmac.h
- LL_HMAC_KEYTYPE_AHB : gr55xx_ll_hmac.h
- LL_HMAC_KEYTYPE_KRAM : gr55xx_ll_hmac.h
- LL_HMAC_KEYTYPE_MCU : gr55xx_ll_hmac.h
- LL_HMAC_ReadReg : gr55xx_ll_hmac.h
- LL_HMAC_WriteReg : gr55xx_ll_hmac.h
- LL_I2C_ABRT_10ADDR1_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_10ADDR2_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_10B_RD_NORSTRT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_7B_ADDR_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_ARB_LOST : gr55xx_ll_i2c.h
- LL_I2C_ABRT_GCALL_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_GCALL_READ : gr55xx_ll_i2c.h
- LL_I2C_ABRT_HS_ACKDET : gr55xx_ll_i2c.h
- LL_I2C_ABRT_HS_NORSTRT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_MST_DIS : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SBYTE_ACKDET : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SBYTE_NORSTRT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SLV_ARBLOST : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SLVFLUSH_TXFIFO : gr55xx_ll_i2c.h
- LL_I2C_ABRT_SLVRD_INTX : gr55xx_ll_i2c.h
- LL_I2C_ABRT_TX_FLUSH_CNT : gr55xx_ll_i2c.h
- LL_I2C_ABRT_TXDATA_NOACK : gr55xx_ll_i2c.h
- LL_I2C_ABRT_USER_ABRT : gr55xx_ll_i2c.h
- LL_I2C_ADDRESSING_MODE_10BIT : gr55xx_ll_i2c.h
- LL_I2C_ADDRESSING_MODE_7BIT : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_GEN_RESTART : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_GEN_STOP : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_READ : gr55xx_ll_i2c.h
- LL_I2C_CMD_MST_WRITE : gr55xx_ll_i2c.h
- LL_I2C_CMD_SLV_NONE : gr55xx_ll_i2c.h
- LL_I2C_DEFAULT_CONFIG : gr55xx_ll_i2c.h
- LL_I2C_DIRECTION_ERROR : gr55xx_ll_i2c.h
- LL_I2C_DIRECTION_NONE : gr55xx_ll_i2c.h
- LL_I2C_DIRECTION_READ : gr55xx_ll_i2c.h
- LL_I2C_DIRECTION_WRITE : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_ACTIVITY : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_ALL : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_GEN_CALL : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_MST_ON_HOLD : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RD_REQ : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RESTART_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_DONE : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_FULL : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_OVER : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_RX_UNDER : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_START_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_STOP_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_TX_ABRT : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_TX_EMPTY : gr55xx_ll_i2c.h
- LL_I2C_INTR_MASK_TX_OVER : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_ACTIVITY : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_GEN_CALL : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_MST_ON_HOLD : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RD_REQ : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RESTART_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_DONE : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_FULL : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_OVER : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_RX_UNDER : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_START_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_STOP_DET : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_TX_ABRT : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_TX_EMPTY : gr55xx_ll_i2c.h
- LL_I2C_INTR_STAT_TX_OVER : gr55xx_ll_i2c.h
- LL_I2C_OWNADDRESS_10BIT : gr55xx_ll_i2c.h
- LL_I2C_OWNADDRESS_7BIT : gr55xx_ll_i2c.h
- LL_I2C_ReadReg : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_1 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_2 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_3 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_4 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_5 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_6 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_CHAR_7 : gr55xx_ll_i2c.h
- LL_I2C_RX_FIFO_TH_FULL : gr55xx_ll_i2c.h
- LL_I2C_SPEED_1000K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_100K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_2000K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_400K : gr55xx_ll_i2c.h
- LL_I2C_SPEED_MODE_FAST : gr55xx_ll_i2c.h
- LL_I2C_SPEED_MODE_HIGH : gr55xx_ll_i2c.h
- LL_I2C_SPEED_MODE_STANDARD : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_1 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_2 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_3 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_4 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_5 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_6 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_CHAR_7 : gr55xx_ll_i2c.h
- LL_I2C_TX_FIFO_TH_EMPTY : gr55xx_ll_i2c.h
- LL_I2C_WriteReg : gr55xx_ll_i2c.h
- LL_I2S_APB_WIDTH_16BIT : gr55xx_ll_i2s.h
- LL_I2S_APB_WIDTH_32BIT : gr55xx_ll_i2s.h
- LL_I2S_APB_WIDTH_8BIT : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_1 : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_2 : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_3 : gr55xx_ll_i2s.h
- LL_I2S_CHANNEL_NUM_4 : gr55xx_ll_i2s.h
- LL_I2S_CLOCK_SRC_32M : gr55xx_ll_i2s.h
- LL_I2S_CLOCK_SRC_96M : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_12BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_16BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_20BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_24BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_32BIT : gr55xx_ll_i2s.h
- LL_I2S_DATASIZE_IGNORE : gr55xx_ll_i2s.h
- LL_I2S_DEFAULT_CONFIG : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_16 : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_2 : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_4 : gr55xx_ll_i2s.h
- LL_I2S_FIFO_DEPTH_8 : gr55xx_ll_i2s.h
- LL_I2S_FULL_DUPLEX : gr55xx_ll_i2s.h
- LL_I2S_INT_RXDA : gr55xx_ll_i2s.h
- LL_I2S_INT_RXFO : gr55xx_ll_i2s.h
- LL_I2S_INT_TXFE : gr55xx_ll_i2s.h
- LL_I2S_INT_TXFO : gr55xx_ll_i2s.h
- LL_I2S_ReadReg : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_12BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_16BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_20BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_24BIT : gr55xx_ll_i2s.h
- LL_I2S_RESOLUTION_32BIT : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_12 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_16 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_20 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_CYCLES_24 : gr55xx_ll_i2s.h
- LL_I2S_SCLKG_NONE : gr55xx_ll_i2s.h
- LL_I2S_SIMPLEX_RX : gr55xx_ll_i2s.h
- LL_I2S_SIMPLEX_TX : gr55xx_ll_i2s.h
- LL_I2S_STATUS_RXDA : gr55xx_ll_i2s.h
- LL_I2S_STATUS_RXFO : gr55xx_ll_i2s.h
- LL_I2S_STATUS_TXFE : gr55xx_ll_i2s.h
- LL_I2S_STATUS_TXFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_10FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_11FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_12FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_13FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_14FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_15FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_16FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_1FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_2FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_3FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_4FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_5FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_6FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_7FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_8FIFO : gr55xx_ll_i2s.h
- LL_I2S_THRESHOLD_9FIFO : gr55xx_ll_i2s.h
- LL_I2S_WriteReg : gr55xx_ll_i2s.h
- LL_I2S_WS_CYCLES_16 : gr55xx_ll_i2s.h
- LL_I2S_WS_CYCLES_24 : gr55xx_ll_i2s.h
- LL_I2S_WS_CYCLES_32 : gr55xx_ll_i2s.h
- LL_ISO7816_ACTION_NONE : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_OFF : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_ON : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_STOPCLK : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_TX : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_TXRX : gr55xx_ll_iso7816.h
- LL_ISO7816_ACTION_WARMRST : gr55xx_ll_iso7816.h
- LL_ISO7816_CARD_ABSENT : gr55xx_ll_iso7816.h
- LL_ISO7816_CARD_PRESENT : gr55xx_ll_iso7816.h
- LL_ISO7816_CLKSTOP_HIGH : gr55xx_ll_iso7816.h
- LL_ISO7816_CLKSTOP_LOW : gr55xx_ll_iso7816.h
- LL_ISO7816_CODING_DEFAULT : gr55xx_ll_iso7816.h
- LL_ISO7816_CODING_INVERSE : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_DMA_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_DONE : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_MASK_ALL : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_PRESENCE : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_RETRY_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_RX_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_STATE_ERR : gr55xx_ll_iso7816.h
- LL_ISO7816_INTR_TEST : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_IDLE : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_OFF : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_RX_WAIT : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_TX : gr55xx_ll_iso7816.h
- LL_ISO7816_IO_STATE_TX_GUARD : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_IDLE : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_OFF : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRDN_RST : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRDN_VCC : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRUP_RST : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_PWRUP_VCC : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_RX_TS0 : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_RX_TS1 : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_STOP : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_STOP_POST : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_STOP_PRE : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_TX : gr55xx_ll_iso7816.h
- LL_ISO7816_PWR_STATE_TX_RX : gr55xx_ll_iso7816.h
- LL_ISO7816_ReadReg : gr55xx_ll_iso7816.h
- LL_ISO7816_WriteReg : gr55xx_ll_iso7816.h
- LL_MSIO_DEFAULT_CONFIG : gr55xx_ll_msio.h
- LL_MSIO_DIRECTION_INOUT : gr55xx_ll_msio.h
- LL_MSIO_DIRECTION_INPUT : gr55xx_ll_msio.h
- LL_MSIO_DIRECTION_NONE : gr55xx_ll_msio.h
- LL_MSIO_DIRECTION_OUTPUT : gr55xx_ll_msio.h
- LL_MSIO_MODE_ANALOG : gr55xx_ll_msio.h
- LL_MSIO_MODE_DIGITAL : gr55xx_ll_msio.h
- LL_MSIO_MUX_0 : gr55xx_ll_msio.h
- LL_MSIO_MUX_1 : gr55xx_ll_msio.h
- LL_MSIO_MUX_2 : gr55xx_ll_msio.h
- LL_MSIO_MUX_3 : gr55xx_ll_msio.h
- LL_MSIO_MUX_4 : gr55xx_ll_msio.h
- LL_MSIO_MUX_5 : gr55xx_ll_msio.h
- LL_MSIO_MUX_6 : gr55xx_ll_msio.h
- LL_MSIO_MUX_7 : gr55xx_ll_msio.h
- LL_MSIO_PIN_0 : gr55xx_ll_msio.h
- LL_MSIO_PIN_1 : gr55xx_ll_msio.h
- LL_MSIO_PIN_2 : gr55xx_ll_msio.h
- LL_MSIO_PIN_3 : gr55xx_ll_msio.h
- LL_MSIO_PIN_4 : gr55xx_ll_msio.h
- LL_MSIO_PIN_ALL : gr55xx_ll_msio.h
- LL_MSIO_PULL_DOWN : gr55xx_ll_msio.h
- LL_MSIO_PULL_NO : gr55xx_ll_msio.h
- LL_MSIO_PULL_UP : gr55xx_ll_msio.h
- LL_MSIO_ReadReg : gr55xx_ll_msio.h
- LL_MSIO_WriteReg : gr55xx_ll_msio.h
- LL_PKC_BIGMULTI_BITS_LENGTH_MAX : gr55xx_ll_pkc.h
- LL_PKC_BITS_LENGTH_MAX : gr55xx_ll_pkc.h
- LL_PKC_BITS_LENGTH_MIN : gr55xx_ll_pkc.h
- LL_PKC_INTEN_BAOVF : gr55xx_ll_pkc.h
- LL_PKC_INTEN_DONE : gr55xx_ll_pkc.h
- LL_PKC_INTEN_ERR : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_ADD : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_BIGINTEGERADD : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_BIGINTEGERMULTIPLY : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_COMPARE : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_INVERTION : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_LEFTSHIFT : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_MULTIPLY : gr55xx_ll_pkc.h
- LL_PKC_operation_mode_SUB : gr55xx_ll_pkc.h
- LL_PKC_ReadReg : gr55xx_ll_pkc.h
- LL_PKC_WORKSTAT_BUSY : gr55xx_ll_pkc.h
- LL_PKC_WriteReg : gr55xx_ll_pkc.h
- LL_PWM_ACTIONEVENT_CLEAR : gr55xx_ll_pwm.h
- LL_PWM_ACTIONEVENT_NONE : gr55xx_ll_pwm.h
- LL_PWM_ACTIONEVENT_SET : gr55xx_ll_pwm.h
- LL_PWM_ACTIONEVENT_TOGGLE : gr55xx_ll_pwm.h
- LL_PWM_BREATH_MODE : gr55xx_ll_pwm.h
- LL_PWM_BREATH_PRESCALER_UNIT : gr55xx_ll_pwm.h
- LL_PWM_CENTER_ALIGNED : gr55xx_ll_pwm.h
- LL_PWM_CHANNEL_DEFAULT_CONFIG : gr55xx_ll_pwm.h
- LL_PWM_DEFAULT_CONFIG : gr55xx_ll_pwm.h
- LL_PWM_DRIVEPOLARITY_NEGATIVE : gr55xx_ll_pwm.h
- LL_PWM_DRIVEPOLARITY_POSITIVE : gr55xx_ll_pwm.h
- LL_PWM_EDGE_ALIGNED : gr55xx_ll_pwm.h
- LL_PWM_FLICKER_MODE : gr55xx_ll_pwm.h
- LL_PWM_HOLD_PRESCALER_UNIT : gr55xx_ll_pwm.h
- LL_PWM_PRESCALER_UNIT : gr55xx_ll_pwm.h
- LL_PWM_ReadReg : gr55xx_ll_pwm.h
- LL_PWM_WriteReg : gr55xx_ll_pwm.h
- LL_PWR_CMD_32_TIMER_LD : gr55xx_ll_pwr.h
- LL_PWR_CMD_DEEP_SLEEP : gr55xx_ll_pwr.h
- LL_PWR_CMD_DPAD_LE_HI : gr55xx_ll_pwr.h
- LL_PWR_CMD_DPAD_LE_LO : gr55xx_ll_pwr.h
- LL_PWR_CMD_EF_DIR_OFF : gr55xx_ll_pwr.h
- LL_PWR_CMD_EF_DIR_ON : gr55xx_ll_pwr.h
- LL_PWR_CMD_EXT_CLK : gr55xx_ll_pwr.h
- LL_PWR_CMD_LD_MEM_SLP_CFG : gr55xx_ll_pwr.h
- LL_PWR_CMD_LD_MEM_WKUP_CFG : gr55xx_ll_pwr.h
- LL_PWR_CMD_LOOPBACK : gr55xx_ll_pwr.h
- LL_PWR_CMD_RNG2_CLK : gr55xx_ll_pwr.h
- LL_PWR_CMD_RNG_CLK : gr55xx_ll_pwr.h
- LL_PWR_CMD_RTC_CLK : gr55xx_ll_pwr.h
- LL_PWR_CMD_SLP_TIMER_MODE_DISABLE : gr55xx_ll_pwr.h
- LL_PWR_CMD_SLP_TIMER_MODE_NORMAL : gr55xx_ll_pwr.h
- LL_PWR_CMD_SLP_TIMER_MODE_RELOAD : gr55xx_ll_pwr.h
- LL_PWR_CMD_SLP_TIMER_MODE_SINGLE : gr55xx_ll_pwr.h
- LL_PWR_DPAD_LE_OFF : gr55xx_ll_pwr.h
- LL_PWR_DPAD_LE_ON : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_INVERT_LSB : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN0 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN1 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN2 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN3 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN4 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN5 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN6 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN7 : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_PIN_ALL : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_SRC_EN_LSB : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_FALLING : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_HIGH : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_LOW : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_LSB : gr55xx_ll_pwr.h
- LL_PWR_EXTWKUP_TYPE_RISING : gr55xx_ll_pwr.h
- LL_PWR_ReadReg : gr55xx_ll_pwr.h
- LL_PWR_TIMER_READ_SEL_AON_WDT : gr55xx_ll_pwr.h
- LL_PWR_TIMER_READ_SEL_CAL_ALARM : gr55xx_ll_pwr.h
- LL_PWR_TIMER_READ_SEL_CAL_TIMER : gr55xx_ll_pwr.h
- LL_PWR_TIMER_READ_SEL_SLP_TIMER : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_ALL : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_BLE : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_BOD_FEDGE : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_CALENDAR : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_EXT : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_MSIO_COMP : gr55xx_ll_pwr.h
- LL_PWR_WKUP_COND_TIMER : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_ALL : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_BLE : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_BOD_FEDGE : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_CALENDAR : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_EXT : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_MSIO_COMP : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_TIMER : gr55xx_ll_pwr.h
- LL_PWR_WKUP_EVENT_WDT : gr55xx_ll_pwr.h
- LL_PWR_WriteReg : gr55xx_ll_pwr.h
- LL_QSPI_DEFAULT_CONFIG : gr55xx_ll_spi.h
- LL_RNG_IT_DISABLE : gr55xx_ll_rng.h
- LL_RNG_IT_ENABLE : gr55xx_ll_rng.h
- LL_RNG_LFSR_MODE_128BIT : gr55xx_ll_rng.h
- LL_RNG_LFSR_MODE_59BIT : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_CYCLIC : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_CYCLIC_PARITY : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_FR0_S0 : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_LFSR : gr55xx_ll_rng.h
- LL_RNG_OUTPUT_LFSR_RNG : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_COUNTING : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_NEUMANN : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_NOT : gr55xx_ll_rng.h
- LL_RNG_POST_PRO_SKIPPING : gr55xx_ll_rng.h
- LL_RNG_ReadReg : gr55xx_ll_rng.h
- LL_RNG_SEED_FR0_S0 : gr55xx_ll_rng.h
- LL_RNG_SEED_USER : gr55xx_ll_rng.h
- LL_RNG_WriteReg : gr55xx_ll_rng.h
- LL_SPI_ReadReg : gr55xx_ll_spi.h
- LL_SPI_WriteReg : gr55xx_ll_spi.h
- LL_SPIM_DEFAULT_CONFIG : gr55xx_ll_spi.h
- LL_SPIS_DEFAULT_CONFIG : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_0BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_12BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_16BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_20BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_24BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_28BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_32BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_36BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_40BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_44BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_48BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_4BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_52BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_56BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_60BIT : gr55xx_ll_spi.h
- LL_SSI_ADDRSIZE_8BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_10BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_11BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_12BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_13BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_14BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_15BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_16BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_17BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_18BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_19BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_20BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_21BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_22BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_23BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_24BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_25BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_26BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_27BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_28BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_29BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_30BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_31BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_32BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_4BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_5BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_6BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_7BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_8BIT : gr55xx_ll_spi.h
- LL_SSI_DATASIZE_9BIT : gr55xx_ll_spi.h
- LL_SSI_DMA_RX_DIS : gr55xx_ll_spi.h
- LL_SSI_DMA_RX_EN : gr55xx_ll_spi.h
- LL_SSI_DMA_TX_DIS : gr55xx_ll_spi.h
- LL_SSI_DMA_TX_EN : gr55xx_ll_spi.h
- LL_SSI_FRF_DUALSPI : gr55xx_ll_spi.h
- LL_SSI_FRF_QUADSPI : gr55xx_ll_spi.h
- LL_SSI_FRF_SPI : gr55xx_ll_spi.h
- LL_SSI_FULL_DUPLEX : gr55xx_ll_spi.h
- LL_SSI_IM_MST : gr55xx_ll_spi.h
- LL_SSI_IM_RXF : gr55xx_ll_spi.h
- LL_SSI_IM_RXO : gr55xx_ll_spi.h
- LL_SSI_IM_RXU : gr55xx_ll_spi.h
- LL_SSI_IM_TXE : gr55xx_ll_spi.h
- LL_SSI_IM_TXO : gr55xx_ll_spi.h
- LL_SSI_INST_ADDR_ALL_IN_SPI : gr55xx_ll_spi.h
- LL_SSI_INST_ADDR_ALL_IN_SPIFRF : gr55xx_ll_spi.h
- LL_SSI_INST_IN_SPI_ADDR_IN_SPIFRF : gr55xx_ll_spi.h
- LL_SSI_INSTSIZE_0BIT : gr55xx_ll_spi.h
- LL_SSI_INSTSIZE_16BIT : gr55xx_ll_spi.h
- LL_SSI_INSTSIZE_4BIT : gr55xx_ll_spi.h
- LL_SSI_INSTSIZE_8BIT : gr55xx_ll_spi.h
- LL_SSI_IS_MST : gr55xx_ll_spi.h
- LL_SSI_IS_RXF : gr55xx_ll_spi.h
- LL_SSI_IS_RXO : gr55xx_ll_spi.h
- LL_SSI_IS_RXU : gr55xx_ll_spi.h
- LL_SSI_IS_TXE : gr55xx_ll_spi.h
- LL_SSI_IS_TXO : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_HANDSHAKE_DIS : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_HANDSHAKE_EN : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_NON_SEQUENTIAL : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_RX : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_SEQUENTIAL : gr55xx_ll_spi.h
- LL_SSI_MICROWIRE_TX : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_10BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_11BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_12BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_13BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_14BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_15BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_16BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_1BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_2BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_3BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_4BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_5BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_6BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_7BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_8BIT : gr55xx_ll_spi.h
- LL_SSI_MW_CMDSIZE_9BIT : gr55xx_ll_spi.h
- LL_SSI_NORMAL_MODE : gr55xx_ll_spi.h
- LL_SSI_PROTOCOL_MICROWIRE : gr55xx_ll_spi.h
- LL_SSI_PROTOCOL_MOTOROLA : gr55xx_ll_spi.h
- LL_SSI_PROTOCOL_TI : gr55xx_ll_spi.h
- LL_SSI_READ_EEPROM : gr55xx_ll_spi.h
- LL_SSI_RIS_MST : gr55xx_ll_spi.h
- LL_SSI_RIS_RXF : gr55xx_ll_spi.h
- LL_SSI_RIS_RXO : gr55xx_ll_spi.h
- LL_SSI_RIS_RXU : gr55xx_ll_spi.h
- LL_SSI_RIS_TXE : gr55xx_ll_spi.h
- LL_SSI_RIS_TXO : gr55xx_ll_spi.h
- LL_SSI_SCPHA_1EDGE : gr55xx_ll_spi.h
- LL_SSI_SCPHA_2EDGE : gr55xx_ll_spi.h
- LL_SSI_SCPOL_HIGH : gr55xx_ll_spi.h
- LL_SSI_SCPOL_LOW : gr55xx_ll_spi.h
- LL_SSI_SIMPLEX_RX : gr55xx_ll_spi.h
- LL_SSI_SIMPLEX_TX : gr55xx_ll_spi.h
- LL_SSI_SLAVE0 : gr55xx_ll_spi.h
- LL_SSI_SLAVE1 : gr55xx_ll_spi.h
- LL_SSI_SLAVE_OUTDIS : gr55xx_ll_spi.h
- LL_SSI_SLAVE_OUTEN : gr55xx_ll_spi.h
- LL_SSI_SR_BUSY : gr55xx_ll_spi.h
- LL_SSI_SR_DCOL : gr55xx_ll_spi.h
- LL_SSI_SR_RFF : gr55xx_ll_spi.h
- LL_SSI_SR_RFNE : gr55xx_ll_spi.h
- LL_SSI_SR_TFE : gr55xx_ll_spi.h
- LL_SSI_SR_TFNF : gr55xx_ll_spi.h
- LL_SSI_SR_TXE : gr55xx_ll_spi.h
- LL_SSI_TEST_MODE : gr55xx_ll_spi.h
- LL_TIMER_ReadReg : gr55xx_ll_tim.h
- LL_TIMER_WriteReg : gr55xx_ll_tim.h
- LL_UART_CTSPIN_STATE_ACTIVE : gr55xx_ll_uart.h
- LL_UART_CTSPIN_STATE_INACTIVE : gr55xx_ll_uart.h
- LL_UART_DATABITS_5B : gr55xx_ll_uart.h
- LL_UART_DATABITS_6B : gr55xx_ll_uart.h
- LL_UART_DATABITS_7B : gr55xx_ll_uart.h
- LL_UART_DATABITS_8B : gr55xx_ll_uart.h
- LL_UART_DEFAULT_CONFIG : gr55xx_ll_uart.h
- LL_UART_HWCONTROL_NONE : gr55xx_ll_uart.h
- LL_UART_HWCONTROL_RTS_CTS : gr55xx_ll_uart.h
- LL_UART_IER_MS : gr55xx_ll_uart.h
- LL_UART_IER_RDA : gr55xx_ll_uart.h
- LL_UART_IER_RLS : gr55xx_ll_uart.h
- LL_UART_IER_THRE : gr55xx_ll_uart.h
- LL_UART_IIR_CTO : gr55xx_ll_uart.h
- LL_UART_IIR_MS : gr55xx_ll_uart.h
- LL_UART_IIR_NIP : gr55xx_ll_uart.h
- LL_UART_IIR_RDA : gr55xx_ll_uart.h
- LL_UART_IIR_RLS : gr55xx_ll_uart.h
- LL_UART_IIR_THRE : gr55xx_ll_uart.h
- LL_UART_LSR_BI : gr55xx_ll_uart.h
- LL_UART_LSR_FE : gr55xx_ll_uart.h
- LL_UART_LSR_OE : gr55xx_ll_uart.h
- LL_UART_LSR_PE : gr55xx_ll_uart.h
- LL_UART_LSR_RFE : gr55xx_ll_uart.h
- LL_UART_LSR_TEMT : gr55xx_ll_uart.h
- LL_UART_LSR_THRE : gr55xx_ll_uart.h
- LL_UART_PARITY_EVEN : gr55xx_ll_uart.h
- LL_UART_PARITY_NONE : gr55xx_ll_uart.h
- LL_UART_PARITY_ODD : gr55xx_ll_uart.h
- LL_UART_PARITY_SP0 : gr55xx_ll_uart.h
- LL_UART_PARITY_SP1 : gr55xx_ll_uart.h
- LL_UART_ReadReg : gr55xx_ll_uart.h
- LL_UART_RTSPIN_STATE_ACTIVE : gr55xx_ll_uart.h
- LL_UART_RTSPIN_STATE_INACTIVE : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_CHAR_1 : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_FULL_2 : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_HALF_FULL : gr55xx_ll_uart.h
- LL_UART_RX_FIFO_TH_QUARTER_FULL : gr55xx_ll_uart.h
- LL_UART_STOPBITS_1 : gr55xx_ll_uart.h
- LL_UART_STOPBITS_1_5 : gr55xx_ll_uart.h
- LL_UART_STOPBITS_2 : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_CHAR_2 : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_EMPTY : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_HALF_FULL : gr55xx_ll_uart.h
- LL_UART_TX_FIFO_TH_QUARTER_FULL : gr55xx_ll_uart.h
- LL_UART_USR_RFF : gr55xx_ll_uart.h
- LL_UART_USR_RFNE : gr55xx_ll_uart.h
- LL_UART_USR_TFE : gr55xx_ll_uart.h
- LL_UART_USR_TFNF : gr55xx_ll_uart.h
- LL_UART_WriteReg : gr55xx_ll_uart.h
- LL_WDT_LOCK_WR_ACCESS_DISABLE : gr55xx_ll_wdt.h
- LL_WDT_LOCK_WR_ACCESS_ENABLE : gr55xx_ll_wdt.h
- LL_WDT_ReadReg : gr55xx_ll_wdt.h
- LL_WDT_WriteReg : gr55xx_ll_wdt.h
- LL_XQSPI_BAUD_RATE_16M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_24M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_32M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_48M : gr55xx_ll_xqspi.h
- LL_XQSPI_BAUD_RATE_64M : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_DIS : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_EN : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_FIFO_CLEAR : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_FIFO_NORMAL : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_HITMISS_CLEAR : gr55xx_ll_xqspi.h
- LL_XQSPI_CACHE_HITMISS_NORMAL : gr55xx_ll_xqspi.h
- LL_XQSPI_DEFAULT_CONFIG : gr55xx_ll_xqspi.h
- LL_XQSPI_DISABLE_PRESENT : gr55xx_ll_xqspi.h
- LL_XQSPI_ENABLE_PRESENT : gr55xx_ll_xqspi.h
- LL_XQSPI_FLASH_WRITE_128BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_FLASH_WRITE_32BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_MODE_QSPI : gr55xx_ll_xqspi.h
- LL_XQSPI_MODE_XIP : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_12BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_16BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_20BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_24BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_28BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_32BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_4BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_DATASIZE_8BIT : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_DEPTH : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_2 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_4 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_1_8 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FIFO_WATERMARK_3_4 : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FRF_DUALSPI : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FRF_QUADSPI : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_FRF_SPI : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_DONE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_RFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_RFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_TFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IM_TFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_DONE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_RFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_RFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_TFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_IS_TFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_LSB : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_MSB : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_BUSY : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_RFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFE : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFF : gr55xx_ll_xqspi.h
- LL_XQSPI_QSPI_STAT_TFTF : gr55xx_ll_xqspi.h
- LL_XQSPI_ReadReg : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPHA_1EDGE : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPHA_2EDGE : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPOL_HIGH : gr55xx_ll_xqspi.h
- LL_XQSPI_SCPOL_LOW : gr55xx_ll_xqspi.h
- LL_XQSPI_WriteReg : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ADDR_3BYTES : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ADDR_4BYTES : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_DUAL_IO_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_DUAL_OUT_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_FAST_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_QUAD_IO_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_QUAD_OUT_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_CMD_READ : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ENDIAN_BIG : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_ENDIAN_LITTLE : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS0 : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS1 : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS2 : gr55xx_ll_xqspi.h
- LL_XQSPI_XIP_SS3 : gr55xx_ll_xqspi.h
- LLS_C_CONNECTION_MAX : lls_c.h
- LNS_CONNECTION_MAX : lns.h
- LNS_LOG_CTRL_PT_VAL_LEN : lns.h
- LNS_LOG_INFO_VAL_LEN : lns.h
- LNS_SERVICE_UUID : lns.h
- LOCAL_INT_DISABLE : gr55xx_hal.h
- LOCAL_INT_RESTORE : gr55xx_hal.h