Data Fields
_ll_uart_init_t Struct Reference
Peripheral Driver » LL Driver » UART » Structures » UART Exported init structures

LL UART init Structure definition. More...

`#include <gr55xx_ll_uart.h>`

## Data Fields
uint32_t | baud_rate
uint32_t | data_bits
uint32_t | stop_bits
uint32_t | parity
uint32_t | hw_flow_ctrl

## Detailed Description

LL UART init Structure definition.

## Field Documentation

## ◆ baud_rate

uint32_t _ll_uart_init_t::baud_rate

This field defines expected Usart communication baud rate.

This feature can be modified afterwards using unitary function ll_uart_set_baud_rate().

## ◆ data_bits

uint32_t _ll_uart_init_t::data_bits

Specifies the number of data bits transmitted or received in a frame. This parameter can be a value of Data Bits.

This feature can be modified afterwards using unitary function ll_uart_set_data_bits_length().

## ◆ hw_flow_ctrl

uint32_t _ll_uart_init_t::hw_flow_ctrl

Specifies whether the hardware flow control mode is enabled or disabled. This parameter can be a value of Hardware Flow Control.

This feature can be modified afterwards using unitary function ll_uart_set_hw_flow_ctrl().

## ◆ parity

uint32_t _ll_uart_init_t::parity

Specifies the parity mode. This parameter can be a value of Parity Control.

This feature can be modified afterwards using unitary function ll_uart_set_parity().

## ◆ stop_bits

uint32_t _ll_uart_init_t::stop_bits

Specifies the number of stop bits transmitted. This parameter can be a value of Stop Bits.

This feature can be modified afterwards using unitary function ll_uart_set_stop_bits_length().

The documentation for this struct was generated from the following file:

- gr55xx_ll_uart.h