Data Fields
app_io_init_t Struct Reference
Peripheral Driver » APP DRIVER » GPIO » Structures

GPIO parameter structure definition. More...

`#include <app_io.h>`

## Data Fields
uint32_t | pin
app_io_mode_t | mode
app_io_pull_t | pull
app_io_mux_t | mux

## Detailed Description

GPIO parameter structure definition.

## Field Documentation

## ◆ mode

app_io_mode_t app_io_init_t::mode

Specifies the operating mode for the selected pins.

## ◆ mux

app_io_mux_t app_io_init_t::mux

Specifies the Peripheral to be connected to the selected pins.

## ◆ pin

uint32_t app_io_init_t::pin

Specifies the IO pins to be configured. This parameter can be any value of IO pins

## ◆ pull

app_io_pull_t app_io_init_t::pull

Specifies the Pull-up or Pull-Down activation for the selected pins.

The documentation for this struct was generated from the following file:

- app_io.h