Here is a list of all documented functions, variables, defines, enums, and typedefs with links to the documentation:

### - r -

- READ : ble_gatts.h
- READ_PERM : ble_gatts.h
- READ_PERM_UNSEC : ble_gatts.h
- READ_POS : ble_gatts.h
- RECEIVE_MAX_LEN : gr55xx_dfu.h
- REMOTE_USER_TERM_CON : ble_l2cap.h
- reslv_rpa_addr_callback_t : ble_gapm.h
- restore_sys_context() : gr55xx_sys.h
- rng_calibration() : gr55xx_sys.h
- rng_handle_t : gr55xx_hal_rng.h
- rng_init_t : gr55xx_hal_rng.h
- RNG_LFSR_MODE_128BIT : gr55xx_hal_rng.h
- RNG_LFSR_MODE_59BIT : gr55xx_hal_rng.h
- RNG_OSC_CLK : platform_sdk.h
- RNG_OSC_CLK2 : platform_sdk.h
- RNG_OUTPUT_CYCLIC : gr55xx_hal_rng.h
- RNG_OUTPUT_CYCLIC_PARITY : gr55xx_hal_rng.h
- RNG_OUTPUT_FR0_S0 : gr55xx_hal_rng.h
- RNG_OUTPUT_LFSR : gr55xx_hal_rng.h
- RNG_OUTPUT_LFSR_RNG : gr55xx_hal_rng.h
- RNG_POST_PRO_COUNTING : gr55xx_hal_rng.h
- RNG_POST_PRO_NEUMANN : gr55xx_hal_rng.h
- RNG_POST_PRO_NOT : gr55xx_hal_rng.h
- RNG_POST_PRO_SKIPPING : gr55xx_hal_rng.h
- RNG_SEED_FR0_S0 : gr55xx_hal_rng.h
- RNG_SEED_USER : gr55xx_hal_rng.h
- rpa_addr_report_callback_t : ble_gapm.h
- RSA_U32_LENGTH : gr55xx_ll_pkc.h
- RSCS_C_CONNECTION_MAX : rscs_c.h
- rscs_c_ctrl_pt_indicate_set() : rscs_c.h
- rscs_c_ctrl_pt_op_code_t : rscs_c.h
- RSCS_C_CTRL_PT_OP_REQ_SUP_LOC : rscs_c.h
- RSCS_C_CTRL_PT_OP_RESERVED : rscs_c.h
- RSCS_C_CTRL_PT_OP_RSP_CODE : rscs_c.h
- RSCS_C_CTRL_PT_OP_SET_CUMUL_VAL : rscs_c.h
- RSCS_C_CTRL_PT_OP_START_CALIB : rscs_c.h
- RSCS_C_CTRL_PT_OP_UPD_LOC : rscs_c.h
- RSCS_C_CTRL_PT_RSP_FAILED : rscs_c.h
- RSCS_C_CTRL_PT_RSP_INVALID_PARAM : rscs_c.h
- RSCS_C_CTRL_PT_RSP_NOT_SUP : rscs_c.h
- RSCS_C_CTRL_PT_RSP_RESERVED : rscs_c.h
- RSCS_C_CTRL_PT_RSP_SUCCESS : rscs_c.h
- rscs_c_ctrl_pt_rsp_t : rscs_c.h
- rscs_c_ctrl_pt_set() : rscs_c.h
- rscs_c_disc_srvc_start() : rscs_c.h
- RSCS_C_ERROR_CCCD_INVALID : rscs_c.h
- RSCS_C_ERROR_PROC_IN_PROGRESS : rscs_c.h
- RSCS_C_EVT_CTRL_PT_IND_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_CTRL_PT_RSP_RECEIVE : rscs_c.h
- RSCS_C_EVT_CTRL_PT_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_DISCOVERY_COMPLETE : rscs_c.h
- RSCS_C_EVT_DISCOVERY_FAIL : rscs_c.h
- rscs_c_evt_handler_t : rscs_c.h
- RSCS_C_EVT_RSC_FEATURE_RECEIVE : rscs_c.h
- RSCS_C_EVT_RSC_MEAS_NTF_SET_SUCCESS : rscs_c.h
- RSCS_C_EVT_RSC_MEAS_VAL_RECEIVE : rscs_c.h
- RSCS_C_EVT_SENSOR_LOC_RECEIVE : rscs_c.h
- rscs_c_evt_type_t : rscs_c.h
- RSCS_C_EVT_WRITE_OP_ERR : rscs_c.h
- RSCS_C_FEAT_CALIBRATION_PROCEDURE_BIT : rscs_c.h
- RSCS_C_FEAT_INSTANT_STRIDE_LEN_BIT : rscs_c.h
- RSCS_C_FEAT_MULTIPLE_SENSORS_BIT : rscs_c.h
- RSCS_C_FEAT_RUNNING_OR_WALKING_STATUS_BIT : rscs_c.h
- RSCS_C_FEAT_TOTAL_DISTANCE_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_INST_STRIDE_LEN_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_RUNNING_OR_WALKING_BIT : rscs_c.h
- RSCS_C_MEAS_FLAG_TOTAL_DISTANCE_BIT : rscs_c.h
- RSCS_C_PT_RSP_LEN_MAX : rscs_c.h
- rscs_c_rsc_feature_read() : rscs_c.h
- rscs_c_rsc_meas_notify_set() : rscs_c.h
- RSCS_C_SENSOR_LOC_FRONT_HUB : rscs_c.h
- RSCS_C_SENSOR_LOC_FRONT_WHEEL : rscs_c.h
- RSCS_C_SENSOR_LOC_HIP : rscs_c.h
- RSCS_C_SENSOR_LOC_LEFT_PEDAL : rscs_c.h
- RSCS_C_SENSOR_LOC_OTHER : rscs_c.h
- rscs_c_sensor_loc_read() : rscs_c.h
- RSCS_C_SENSOR_LOC_RIGHT_PEDAL : rscs_c.h
- RSCS_C_SENSOR_LOC_SHOE_IN : rscs_c.h
- RSCS_C_SENSOR_LOC_SHOE_TOP : rscs_c.h
- RSCS_C_SENSOR_LOC_SUP_NB : rscs_c.h
- rscs_c_sensor_loc_t : rscs_c.h
- RSCS_CHAR_FULL : rscs.h
- RSCS_CHAR_MANDATORY : rscs.h
- RSCS_CHAR_SC_CTRL_POINT : rscs.h
- RSCS_CHAR_SENSOR_LOC_SUP : rscs.h
- rscs_client_init() : rscs_c.h
- RSCS_CONNECTION_MAX : rscs.h
- rscs_ctrl_pt_op_code_t : rscs.h
- RSCS_CTRL_PT_OP_REQ_SUP_LOC : rscs.h
- RSCS_CTRL_PT_OP_RESERVED : rscs.h
- RSCS_CTRL_PT_OP_RSP_CODE : rscs.h
- RSCS_CTRL_PT_OP_SET_CUMUL_VAL : rscs.h
- RSCS_CTRL_PT_OP_START_CALIB : rscs.h
- RSCS_CTRL_PT_OP_UPD_LOC : rscs.h
- RSCS_CTRL_PT_RSP_FAILED : rscs.h
- RSCS_CTRL_PT_RSP_INVALID_PARAM : rscs.h
- RSCS_CTRL_PT_RSP_LEN_MIN : rscs.h
- RSCS_CTRL_PT_RSP_NOT_SUP : rscs.h
- RSCS_CTRL_PT_RSP_RESERVED : rscs.h
- rscs_ctrl_pt_rsp_send() : rscs.h
- RSCS_CTRL_PT_RSP_SUCCESS : rscs.h
- rscs_ctrl_pt_rsp_t : rscs.h
- RSCS_CTRL_PT_VAL_LEN_MAX : rscs.h
- RSCS_ERROR_CCCD_INVALID : rscs.h
- RSCS_ERROR_PROC_IN_PROGRESS : rscs.h
- RSCS_EVT_CTRL_POINT_INDICATION_DISABLE : rscs.h
- RSCS_EVT_CTRL_POINT_INDICATION_ENABLE : rscs.h
- RSCS_EVT_CTRL_POINT_RSP_CPLT : rscs.h
- RSCS_EVT_CUMUL_VAL_SET : rscs.h
- rscs_evt_handler_t : rscs.h
- RSCS_EVT_INVALID : rscs.h
- RSCS_EVT_RSC_MEAS_NOTIFICATION_DISABLE : rscs.h
- RSCS_EVT_RSC_MEAS_NOTIFICATION_ENABLE : rscs.h
- RSCS_EVT_RSC_MEAS_SEND_CPLT : rscs.h
- RSCS_EVT_SEBSOR_CALIBRATION : rscs.h
- RSCS_EVT_SEBSOR_LOC_UPD : rscs.h
- RSCS_EVT_SUP_SEBSOR_LOC_REQ : rscs.h
- rscs_evt_type_t : rscs.h
- RSCS_FEAR_FULL_BIT : rscs.h
- RSCS_FEAT_CALIBRATION_PROCEDURE_BIT : rscs.h
- RSCS_FEAT_INSTANT_STRIDE_LEN_BIT : rscs.h
- RSCS_FEAT_MULTIPLE_SENSORS_BIT : rscs.h
- RSCS_FEAT_RUNNING_OR_WALKING_STATUS_BIT : rscs.h
- RSCS_FEAT_TOTAL_DISTANCE_BIT : rscs.h
- RSCS_FEAT_VAL_LEN_MAX : rscs.h
- RSCS_MEAS_FLAG_INST_STRIDE_LEN_BIT : rscs.h
- RSCS_MEAS_FLAG_RUNNING_OR_WALKING_BIT : rscs.h
- RSCS_MEAS_FLAG_TOTAL_DISTANCE_BIT : rscs.h
- RSCS_MEAS_VAL_LEN_MAX : rscs.h
- rscs_measurement_send() : rscs.h
- RSCS_SENSOR_LOC_FRONT_HUB : rscs.h
- RSCS_SENSOR_LOC_FRONT_WHEEL : rscs.h
- RSCS_SENSOR_LOC_HIP : rscs.h
- RSCS_SENSOR_LOC_LEFT_PEDAL : rscs.h
- RSCS_SENSOR_LOC_OTHER : rscs.h
- RSCS_SENSOR_LOC_RIGHT_PEDAL : rscs.h
- RSCS_SENSOR_LOC_SHOE_IN : rscs.h
- RSCS_SENSOR_LOC_SHOE_TOP : rscs.h
- RSCS_SENSOR_LOC_SUP_NB : rscs.h
- rscs_sensor_loc_t : rscs.h
- rscs_sensor_loc_update() : rscs.h
- RSCS_SENSOR_LOC_VAL_LEN_MAX : rscs.h
- rscs_service_init() : rscs.h
- rtc_calibration() : gr55xx_sys.h
- RTC_OSC_CLK : platform_sdk.h
- RTUS_CHAR_FULL : rtus.h
- RTUS_CONNECTION_MAX : rtus.h
- RTUS_CTRL_PT_CANCEL_UPDATE : rtus.h
- RTUS_CTRL_PT_GET_UPDATE : rtus.h
- rtus_ctrl_pt_t : rtus.h
- RTUS_CTRL_PT_VAL_LEN : rtus.h
- RTUS_CUR_STATE_IDLE : rtus.h
- RTUS_CUR_STATE_PENDING : rtus.h
- rtus_cur_state_t : rtus.h
- rtus_current_state_set() : rtus.h
- RTUS_EVT_CANCEL_UPDATE : rtus.h
- RTUS_EVT_GET_UPDATE : rtus.h
- rtus_evt_handler_t : rtus.h
- RTUS_EVT_INVALID : rtus.h
- rtus_evt_type_t : rtus.h
- rtus_service_init() : rtus.h
- RTUS_UPDATE_RESULT_CANCELED : rtus.h
- RTUS_UPDATE_RESULT_NO_ATTEMPTED : rtus.h
- RTUS_UPDATE_RESULT_NO_CONN_TO_REF : rtus.h
- RTUS_UPDATE_RESULT_REP_ERROR : rtus.h
- RTUS_UPDATE_RESULT_SCCESSFUL : rtus.h
- rtus_update_result_set() : rtus.h
- rtus_update_result_t : rtus.h
- RTUS_UPDATE_RESULT_TIMEOUT : rtus.h
- RTUS_UPDATE_STATE_VAL_LEN : rtus.h
- run_mode_t : platform_sdk.h
- rx_handler_cb_t : gr55xx_lcp.h , lcp_sdk.h