Macros
AON_GPIO pins
Peripheral Driver » HAL Driver » AON_GPIO » Defines » AON_GPIO Exported Constants

## Macros
#define | AON_GPIO_PIN_0 ((uint16_t)0x0001U)
#define | AON_GPIO_PIN_1 ((uint16_t)0x0002U)
#define | AON_GPIO_PIN_2 ((uint16_t)0x0004U)
#define | AON_GPIO_PIN_3 ((uint16_t)0x0008U)
#define | AON_GPIO_PIN_4 ((uint16_t)0x0010U)
#define | AON_GPIO_PIN_5 ((uint16_t)0x0020U)
#define | AON_GPIO_PIN_6 ((uint16_t)0x0040U)
#define | AON_GPIO_PIN_7 ((uint16_t)0x0080U)
#define | AON_GPIO_PIN_ALL ((uint16_t)0x00FFU)
#define | AON_GPIO_PIN_MASK (0x000000FFU)

## Detailed Description

## Macro Definition Documentation

## ◆ AON_GPIO_PIN_0

#define AON_GPIO_PIN_0 ((uint16_t)0x0001U)

Pin 0 selected

## ◆ AON_GPIO_PIN_1

#define AON_GPIO_PIN_1 ((uint16_t)0x0002U)

Pin 1 selected

## ◆ AON_GPIO_PIN_2

#define AON_GPIO_PIN_2 ((uint16_t)0x0004U)

Pin 2 selected

## ◆ AON_GPIO_PIN_3

#define AON_GPIO_PIN_3 ((uint16_t)0x0008U)

Pin 3 selected

## ◆ AON_GPIO_PIN_4

#define AON_GPIO_PIN_4 ((uint16_t)0x0010U)

Pin 4 selected

## ◆ AON_GPIO_PIN_5

#define AON_GPIO_PIN_5 ((uint16_t)0x0020U)

Pin 5 selected

## ◆ AON_GPIO_PIN_6

#define AON_GPIO_PIN_6 ((uint16_t)0x0040U)

Pin 6 selected

## ◆ AON_GPIO_PIN_7

#define AON_GPIO_PIN_7 ((uint16_t)0x0080U)

Pin 7 selected

## ◆ AON_GPIO_PIN_ALL

#define AON_GPIO_PIN_ALL ((uint16_t)0x00FFU)

All pins selected

## ◆ AON_GPIO_PIN_MASK

#define AON_GPIO_PIN_MASK (0x000000FFU)

PIN mask for assert test