Functions
DMA_Management
Peripheral Driver » LL Driver » UART » Functions

## Functions
__STATIC_INLINE uint32_t | ll_uart_dma_get_register_address (uart_regs_t *UARTx)
| Get the data register address used for DMA transfer. More...

## Detailed Description

## Function Documentation

## ◆ ll_uart_dma_get_register_address()

__STATIC_INLINE uint32_t ll_uart_dma_get_register_address | ( | uart_regs_t * | UARTx | ) |

Get the data register address used for DMA transfer.

Note
  The address of data register RBR is the same as the address of THR.

Register | BitsName
--- | ---
RBR | RBR
THR | THR

Parameters

  UARTx | UART instance

Return values

  Address | of data register