Data Fields
pass_c_handles_t Struct Reference
BLE Services » Phone Alert Status Service Client (PASS_C) » Structures

Handles on the connected peer device needed to interact with it. More...

`#include <pass_c.h>`

## Data Fields
uint16_t | pass_srvc_start_handle
uint16_t | pass_srvc_end_handle
uint16_t | pass_alert_status_handle
uint16_t | pass_alert_status_cccd_handle
uint16_t | pass_ringer_set_handle
uint16_t | pass_ringer_set_cccd_handle
uint16_t | pass_ringer_ctrl_pt_handle

## Detailed Description

Handles on the connected peer device needed to interact with it.

## Field Documentation

## ◆ pass_alert_status_cccd_handle

uint16_t pass_c_handles_t::pass_alert_status_cccd_handle

PASS CCCD handle of Alert Status characteristic which has been got from peer.

## ◆ pass_alert_status_handle

uint16_t pass_c_handles_t::pass_alert_status_handle

PASS Alert Status characteristic Value handle which has been got from peer.

## ◆ pass_ringer_ctrl_pt_handle

uint16_t pass_c_handles_t::pass_ringer_ctrl_pt_handle

PASS Ringer Control Point characteristic Value handle which has been got from peer.

## ◆ pass_ringer_set_cccd_handle

uint16_t pass_c_handles_t::pass_ringer_set_cccd_handle

PASS CCCD handle of Ringer Setting characteristic which has been got from peer.

## ◆ pass_ringer_set_handle

uint16_t pass_c_handles_t::pass_ringer_set_handle

PASS Ringer Setting characteristic Value handle which has been got from peer.

## ◆ pass_srvc_end_handle

uint16_t pass_c_handles_t::pass_srvc_end_handle

PASS Service end handle.

## ◆ pass_srvc_start_handle

uint16_t pass_c_handles_t::pass_srvc_start_handle

PASS Service start handle.

The documentation for this struct was generated from the following file:

- pass_c.h