Data Fields
hrs_c_evt_t Struct Reference
BLE Services » Heart Rate Service Client (HRS_C) » Structures

Heart Rate Service Client event. More...

`#include <hrs_c.h>`

## Data Fields
uint8_t | conn_idx
hrs_c_evt_type_t | evt_type
union {
hrs_c_hr_meas_t hr_meas_buff
hrs_c_sensor_loc_t sensor_loc
} | value

## Detailed Description

Heart Rate Service Client event.

## Field Documentation

## ◆ conn_idx

uint8_t hrs_c_evt_t::conn_idx

The connection index.

## ◆ evt_type

hrs_c_evt_type_t hrs_c_evt_t::evt_type

HRS Client event type.

## ◆ hr_meas_buff

hrs_c_hr_meas_t hrs_c_evt_t::hr_meas_buff

Buffer of heart rate measurement value.

## ◆ sensor_loc

hrs_c_sensor_loc_t hrs_c_evt_t::sensor_loc

Sensor location.

## ◆ value

union { ... } hrs_c_evt_t::value

Decoded result of value received.

The documentation for this struct was generated from the following file:

- hrs_c.h