thscps.h
Go to the documentation of this file.
1 /**
2 *****************************************************************************************
3 *
4 * @file thscps.h
5 *
6 * @brief Throughput Control Point Service API
7 *
8 *****************************************************************************************
9 * @attention
10 #####Copyright (c) 2019 GOODIX
11 All rights reserved.
12
13 Redistribution and use in source and binary forms, with or without
14 modification, are permitted provided that the following conditions are met:
15 * Redistributions of source code must retain the above copyright
16 notice, this list of conditions and the following disclaimer.
17 * Redistributions in binary form must reproduce the above copyright
18 notice, this list of conditions and the following disclaimer in the
19 documentation and/or other materials provided with the distribution.
20 * Neither the name of GOODIX nor the names of its contributors may be used
21 to endorse or promote products derived from this software without
22 specific prior written permission.
23
24 THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
25 AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
26 IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
27 ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
28 LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
29 CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
30 SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
31 INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
32 CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
33 ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
34 POSSIBILITY OF SUCH DAMAGE.
35 *****************************************************************************************
36 */
37
38 /**
39 * @addtogroup BLE_SRV BLE Services
40 * @{
41 * @brief Definitions and prototypes for the BLE Service Interface.
42 */
43
44 /**
45 * @defgroup BLE_SDK_THSCPS Throughput Control Point Client (THSCPS)
46 * @{
47 * @brief THS Control Point Interface module.
48 *
49 * @details The Throughput Control Point Service contains the APIs and types, which can be used by the
50 * application to perform throughput parameters set.
51 *
52 * After \ref thscps_evt_handler_t variable is initialized, the application must call \ref thscps_service_init()
53 * to add the Throughput Control Point Service and THS Control Point, THS Control Point Response characteristics
54 * to the BLE Stack database.
55 */
56
57 #ifndef __THSCPS_H__
58 #define __THSCPS_H__
59
60 #include "ble_prf_types.h"
61 #include "gr55xx_sys.h"
62 #include "custom_config.h"
63
64 /**
65 * @defgroup THSCPS_MACRO Defines
66 * @{
67 */
68 #define THSCPS_CONNECTION_MAX (10 < CFG_MAX_CONNECTIONS ?\
69 10 : CFG_MAX_CONNECTIONS) /**< Maximum number of THSCPS connections. */
70 #define THSCPS_CTRL_PT_VAL_LEN 20 /**< Length of the value of Control Point characteristic. */
71 #define THSCPS_TEST_SETTING_VAL_LEN 20 /**< Length of the value of Test Setting characteristic. */
72 #define THSCPS_TEST_INFO_VAL_LEN 20 /**< Length of the value of Test Information characteristic. */
73 #define THSCPS_CONN_INFO_VAL_LEN 20 /**< Length of the value of Connection Information characteristic. */
74 #define THSCPS_SERVICE_UUID 0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80,\
75 0x0A, 0x46, 0x44, 0xD3, 0x01, 0x07, 0xED, 0xA6 /**< The UUID of THS Control Point Control Point Service for setting advertising data. */
76 #define THSCPS_ACTION_ON 0x01 /**< Start the action. */
77 #define THSCPS_ACTION_OFF 0x00 /**< Stop the action. */
78 #define THSCPS_CTRL_PT_RSP_CODE 0xff /**< Response code. */
79 /** @} */
80
81 /**
82 * @defgroup THSCPS_ENUM Enumerations
83 * @{
84 */
85 /**@brief Local device GAP Role Type. */
86 typedef enum
87 {
88 THSCPS_TEST_ROLE_INVALID, /**< Test role: Invalid. */
89 THSCPS_TEST_ROLE_SLAVE, /**< Test role: Slave. */
90 THSCPS_TEST_ROLE_MASTER, /**< Test role: Master. */
91 } thscps_test_role_t;
92
93 /**
94 * @brief Specify PHY. */
95 typedef enum
96 {
97 THSCPS_LEGACY_ADV_PHY, /**< Undefined LE PHY. */
98 THSCPS_1MBPS_PHY, /**< LE 1M PHY. */
99 THSCPS_CODED_PHY , /**< LE Coded PHY. */
100 } thscps_adv_phy_t;
101
102 /**@brief Throughput Test State. */
103 typedef enum
104 {
105 THSCPS_TEST_STOP, /**< Throughput Test is not ongoing. */
106 THSCPS_TEST_STARTED, /**< Throughput Test is ongoing. */
107 } thscps_test_state_t;
108
109 /**@brief THS Control Point Service Control Point IDs. */
110 typedef enum
111 {
112 THSCPS_CTRL_PT_INVALID, /**< Invalid cmd id. */
113 THSCPS_CTRL_PT_TEST_ROLE, /**< Test role set. */
114 THSCPS_CTRL_PT_ADV_PARAM, /**< Advertising parameters set. */
115 THSCPS_CTRL_PT_ADV_ACTION, /**< Advertiding action. */
116 THSCPS_CTRL_PT_SCAN_ACTION, /**< Scan action. */
117 THSCPS_CTRL_PT_TEST_READY, /**< Ready for test. */
118 THSCPS_CTRL_PT_SETTING,
119 } thscps_ctrl_pt_id_t;
120
121 /**@brief Throughput service settings types. */
122 typedef enum
123 {
124 THSCPS_SETTINGS_TYPE_CI, /**< BLE Connection Interval parameter. */
125 THSCPS_SETTINGS_TYPE_MTU, /**< MTU Size. */
126 THSCPS_SETTINGS_TYPE_PDU, /**< PDU Size. */
127 THSCPS_SETTINGS_TYPE_PHY, /**< Radio Phy mode, 1M, 2M, Encoded. */
128 THSCPS_SETTINGS_TYPE_TRANS_MODE, /**< Data transmission mode. */
129 THSCPS_SETTINGS_TYPE_TX_POWER, /**< Connect Tx power. */
130 THSCPS_SETTINGS_TYPE_TOGGLE, /**< Throughput toggle state of sending the data. */
131 }thscps_settings_type_t;
132
133 /**@brief THS Control Point Response Types. */
134 typedef enum
135 {
136 THSCPS_RSP_ID_SUCCESS, /**< Success. */
137 THSCPS_RSP_ID_UNSUPPORT, /**< Failed because of unsupport command. */
138 THSCPS_RSP_ID_STATUS_ERR, /**< Failed because of disallowed status. */
139 THSCPS_RSP_ID_PARAM_ERR, /**< Failed because of parameter error. */
140 THSCPS_RSP_ID_TEST_ROLE_ERR, /**< Failed becaude of Test role error. */
141 THSCPS_RSP_ID_SDK_ERR, /**< Failed becaude of SDK error Size. */
142 } thscps_status_rsp_t;
143
144 /**@brief THS Control Point Service Event Type. */
145 typedef enum
146 {
147 THSCPS_EVT_INVALID, /**< Throughput Control Point Service invalid event. */
148 THSCPS_EVT_CTRL_PT_IND_ENABLE, /**< THS Control Point indicaiton is enabled. */
149 THSCPS_EVT_CTRL_PT_IND_DISABLE, /**< THS Control Point indicaiton is disabled. */
150 THSCPS_EVT_TSET_SET_NTF_ENABLE, /**< THS Test Information notification is enabled. */
151 THSCPS_EVT_TSET_SET_NTF_DISABLE, /**< THS Test Information notification is disabled. */
152 THSCPS_EVT_TSET_INFO_NTF_ENABLE, /**< THS Test Information notification is enabled. */
153 THSCPS_EVT_TSET_INFO_NTF_DISABLE, /**< THS Test Information notification is disabled. */
154 THSCPS_EVT_CONN_INFO_NTF_ENABLE, /**< THS Connection Information notification is enabled. */
155 THSCPS_EVT_CONN_INFO_NTF_DISABLE, /**< THS Connection Information notification is disabled. */
156 THSCPS_EVT_TEST_ROLE_SET, /**< Set Test role. */
157 THSCPS_EVT_ADV_PRAM_SET, /**< Set advertising parameters. */
158 THSCPS_EVT_ADV_ACTION, /**< Set advertising action. */
159 THSCPS_EVT_SCAN_ACTION, /**< Set scan action. */
160 THSCPS_EVT_SETTING_SET, /**< Throughput setting. */
161 } thscps_evt_type_t;
162 /** @} */
163
164 /**
165 * @defgroup THSCPS_STRUCT Structures
166 * @{
167 */
168 /**@brief THS Setting Information value. */
169 typedef struct
170 {
171 uint16_t length; /**< THS Setting Information length. */
172 const uint8_t *p_data; /**< THS Setting Information data. */
173 } thscps_setting_t;
174
175 /**@brief THS Test Information value. */
176 typedef struct
177 {
178 int8_t rssi; /**< RX rssi. */
179 uint8_t right_rate; /**< RX right rate. */
180 uint16_t instant_val; /**< Instant throughput value. */
181 uint16_t average_val; /**< Average throughput value. */
182 uint16_t packets_val; /**< Recieved Packects value. */
183 } thscps_test_info_t;
184
185 /**@brief THS connect Information value. */
186 typedef struct
187 {
188 uint16_t ci; /**< Connect Interval. */
189 uint16_t pdu; /**< PDU. */
190 uint16_t mtu; /**< MTU. */
191 uint8_t tx_phy; /**< TX PHY. */
192 uint8_t rx_phy; /**< RX PHY. */
193 int8_t tx_power; /**< TX Power. */
194 uint8_t ths_mode; /**< THS Mode. */
195 } thscps_test_conn_info_t;
196
197 /**@brief THS Control Point Advertising Parameters. */
198 typedef struct
199 {
200 thscps_adv_phy_t phy; /**< Specify what PHY the Controller has changed for TX/RX. */
201 uint16_t interval; /**< Advertising interval. */
202 uint16_t duration; /**< Advertising duration. */
203 int8_t tx_power; /**< Advertising tx power. */
204 } thscps_adv_param_t;
205
206 /**@brief THS Control Point Response value. */
207 typedef struct
208 {
209 uint8_t cmd_id; /**< Commander ID. */
210 thscps_status_rsp_t status; /**< Status. */
211 uint8_t conn_idx; /**< Connection of cmd set. */
212 } thscps_rsp_val_t;
213
214 /**@brief THS Control Point Service event. */
215 typedef struct
216 {
217 uint8_t conn_idx; /**< The connection index. */
218 thscps_evt_type_t evt_type; /**< THS client event type. */
219 union
220 {
221 uint8_t action_set; /**< Set action. */
222 thscps_test_role_t test_role; /**< GAP role type. */
223 thscps_adv_param_t adv_param; /**< Advertising parameters. */
224 thscps_setting_t setting_info; /**< Setting infomation. */
225 } param; /**< Event parameters. */
226 } thscps_evt_t;
227 /** @} */
228
229 /**
230 * @defgroup THSCPS_TYPEDEF Typedefs
231 * @{
232 */
233 /**@brief THS Control Point Service event handler type. */
234 typedef void (*thscps_evt_handler_t)(thscps_evt_t *p_evt);
235 /** @} */
236
237 /**
238 * @defgroup THSCPS_FUNCTION Functions
239 * @{
240 */
241 /**
242 *****************************************************************************************
243 * @brief Initialize a THS Control Point Service instance and add in the DB.
244 *
245 * @param[in] evt_handler: THS Control Point Service event handler.
246 *
247 * @return Result of service initialization.
248 *****************************************************************************************
249 */
250 sdk_err_t thscps_service_init(thscps_evt_handler_t evt_handler);
251
252 /**
253 *****************************************************************************************
254 * @brief Send Control Point Response if its indicaiton has been enabled.
255 *
256 * @param[in] conn_idx: Connnection index.
257 * @param[in] p_rsp_val: Pointer to Response value.
258 *
259 * @return Result of indicate value.
260 *****************************************************************************************
261 */
262 sdk_err_t thscps_ctrl_pt_rsp_send(uint8_t conn_idx, thscps_rsp_val_t *p_rsp_val);
263
264 /**
265 *****************************************************************************************
266 * @brief Send Settings Response if its notification has been enabled.
267 *
268 * @param[in] conn_idx: Connnection index.
269 * @param[in] p_rsp_val: Pointer to Response value.
270 *
271 * @return Result of indicate value.
272 *****************************************************************************************
273 */
274 sdk_err_t thscps_test_setting_rsp_send(uint8_t conn_idx, thscps_rsp_val_t *p_rsp_val);
275
276 /**
277 *****************************************************************************************
278 * @brief Send Throughput Test Information if its notification has been enabled.
279 *
280 * @param[in] conn_idx: Connnection index.
281 * @param[in] p_test_info: Pointer to test information value.
282 *
283 * @return Result of notify value.
284 *****************************************************************************************
285 */
286 sdk_err_t thscps_test_info_send(uint8_t conn_idx, thscps_test_info_t *p_test_info);
287
288 /**
289 *****************************************************************************************
290 * @brief Send Throughput Test Connect Information if its notification has been enabled.
291 *
292 * @param[in] conn_idx: Connnection index.
293 * @param[in] p_conn_info: Pointer to connection information value.
294 *
295 * @return Result of notify value.
296 *****************************************************************************************
297 */
298 sdk_err_t thscps_conn_info_send(uint8_t conn_idx, thscps_test_conn_info_t *p_conn_info);
299
300 /**
301 *****************************************************************************************
302 * @brief Set throughput state set.
303 *
304 * @param[in] test_state: Throughput Test state.
305 *****************************************************************************************
306 */
307 void thscps_test_state_set(thscps_test_state_t test_state);
308 /** @} */
309 #endif
310 /** @} */
311 /** @} */
THSCPS_EVT_CTRL_PT_IND_ENABLE
@ THSCPS_EVT_CTRL_PT_IND_ENABLE
THS Control Point indicaiton is enabled.
Definition: thscps.h:148
thscps_evt_t::setting_info
thscps_setting_t setting_info
Setting infomation.
Definition: thscps.h:224
thscps_conn_info_send
sdk_err_t thscps_conn_info_send(uint8_t conn_idx, thscps_test_conn_info_t *p_conn_info)
Send Throughput Test Connect Information if its notification has been enabled.
thscps_adv_param_t::tx_power
int8_t tx_power
Advertising tx power.
Definition: thscps.h:203
thscps_adv_param_t::duration
uint16_t duration
Advertising duration.
Definition: thscps.h:202
THSCPS_TEST_ROLE_MASTER
@ THSCPS_TEST_ROLE_MASTER
Test role: Master.
Definition: thscps.h:90
thscps_service_init
sdk_err_t thscps_service_init(thscps_evt_handler_t evt_handler)
Initialize a THS Control Point Service instance and add in the DB.
THSCPS_LEGACY_ADV_PHY
@ THSCPS_LEGACY_ADV_PHY
Undefined LE PHY.
Definition: thscps.h:97
thscps_adv_phy_t
thscps_adv_phy_t
Specify PHY.
Definition: thscps.h:96
thscps_setting_t::p_data
const uint8_t * p_data
THS Setting Information data.
Definition: thscps.h:172
THSCPS_EVT_TSET_INFO_NTF_ENABLE
@ THSCPS_EVT_TSET_INFO_NTF_ENABLE
THS Test Information notification is enabled.
Definition: thscps.h:152
thscps_test_info_t::right_rate
uint8_t right_rate
RX right rate.
Definition: thscps.h:179
thscps_adv_param_t::interval
uint16_t interval
Advertising interval.
Definition: thscps.h:201
thscps_evt_t
THS Control Point Service event.
Definition: thscps.h:216
THSCPS_SETTINGS_TYPE_PHY
@ THSCPS_SETTINGS_TYPE_PHY
Radio Phy mode, 1M, 2M, Encoded.
Definition: thscps.h:127
THSCPS_CTRL_PT_SCAN_ACTION
@ THSCPS_CTRL_PT_SCAN_ACTION
Scan action.
Definition: thscps.h:116
thscps_test_state_t
thscps_test_state_t
Throughput Test State.
Definition: thscps.h:104
thscps_test_setting_rsp_send
sdk_err_t thscps_test_setting_rsp_send(uint8_t conn_idx, thscps_rsp_val_t *p_rsp_val)
Send Settings Response if its notification has been enabled.
thscps_test_conn_info_t::ci
uint16_t ci
Connect Interval.
Definition: thscps.h:188
THSCPS_EVT_TSET_SET_NTF_DISABLE
@ THSCPS_EVT_TSET_SET_NTF_DISABLE
THS Test Information notification is disabled.
Definition: thscps.h:151
thscps_evt_t::test_role
thscps_test_role_t test_role
GAP role type.
Definition: thscps.h:222
thscps_test_conn_info_t
THS connect Information value.
Definition: thscps.h:187
thscps_evt_t::adv_param
thscps_adv_param_t adv_param
Advertising parameters.
Definition: thscps.h:223
thscps_ctrl_pt_rsp_send
sdk_err_t thscps_ctrl_pt_rsp_send(uint8_t conn_idx, thscps_rsp_val_t *p_rsp_val)
Send Control Point Response if its indicaiton has been enabled.
THSCPS_1MBPS_PHY
@ THSCPS_1MBPS_PHY
LE 1M PHY.
Definition: thscps.h:98
thscps_test_state_set
void thscps_test_state_set(thscps_test_state_t test_state)
Set throughput state set.
thscps_test_info_t::rssi
int8_t rssi
RX rssi.
Definition: thscps.h:178
THSCPS_EVT_TEST_ROLE_SET
@ THSCPS_EVT_TEST_ROLE_SET
Set Test role.
Definition: thscps.h:156
gr55xx_sys.h
GR55XX System API.
thscps_rsp_val_t::status
thscps_status_rsp_t status
Status.
Definition: thscps.h:210
THSCPS_EVT_ADV_PRAM_SET
@ THSCPS_EVT_ADV_PRAM_SET
Set advertising parameters.
Definition: thscps.h:157
THSCPS_RSP_ID_SDK_ERR
@ THSCPS_RSP_ID_SDK_ERR
Failed becaude of SDK error Size.
Definition: thscps.h:141
thscps_status_rsp_t
thscps_status_rsp_t
THS Control Point Response Types.
Definition: thscps.h:135
THSCPS_SETTINGS_TYPE_PDU
@ THSCPS_SETTINGS_TYPE_PDU
PDU Size.
Definition: thscps.h:126
thscps_adv_param_t
THS Control Point Advertising Parameters.
Definition: thscps.h:199
THSCPS_SETTINGS_TYPE_TX_POWER
@ THSCPS_SETTINGS_TYPE_TX_POWER
Connect Tx power.
Definition: thscps.h:129
thscps_test_info_send
sdk_err_t thscps_test_info_send(uint8_t conn_idx, thscps_test_info_t *p_test_info)
Send Throughput Test Information if its notification has been enabled.
thscps_test_info_t
THS Test Information value.
Definition: thscps.h:177
thscps_setting_t::length
uint16_t length
THS Setting Information length.
Definition: thscps.h:171
thscps_test_info_t::average_val
uint16_t average_val
Average throughput value.
Definition: thscps.h:181
THSCPS_RSP_ID_STATUS_ERR
@ THSCPS_RSP_ID_STATUS_ERR
Failed because of disallowed status.
Definition: thscps.h:138
THSCPS_RSP_ID_PARAM_ERR
@ THSCPS_RSP_ID_PARAM_ERR
Failed because of parameter error.
Definition: thscps.h:139
thscps_evt_t::action_set
uint8_t action_set
Set action.
Definition: thscps.h:221
THSCPS_SETTINGS_TYPE_CI
@ THSCPS_SETTINGS_TYPE_CI
BLE Connection Interval parameter.
Definition: thscps.h:124
thscps_test_info_t::instant_val
uint16_t instant_val
Instant throughput value.
Definition: thscps.h:180
THSCPS_CTRL_PT_TEST_READY
@ THSCPS_CTRL_PT_TEST_READY
Ready for test.
Definition: thscps.h:117
THSCPS_RSP_ID_SUCCESS
@ THSCPS_RSP_ID_SUCCESS
Success.
Definition: thscps.h:136
THSCPS_EVT_SCAN_ACTION
@ THSCPS_EVT_SCAN_ACTION
Set scan action.
Definition: thscps.h:159
thscps_test_conn_info_t::mtu
uint16_t mtu
MTU.
Definition: thscps.h:190
thscps_setting_t
THS Setting Information value.
Definition: thscps.h:170
ble_prf_types.h
Profile/Service Common Types.
THSCPS_CTRL_PT_TEST_ROLE
@ THSCPS_CTRL_PT_TEST_ROLE
Test role set.
Definition: thscps.h:113
THSCPS_EVT_TSET_INFO_NTF_DISABLE
@ THSCPS_EVT_TSET_INFO_NTF_DISABLE
THS Test Information notification is disabled.
Definition: thscps.h:153
thscps_settings_type_t
thscps_settings_type_t
Throughput service settings types.
Definition: thscps.h:123
THSCPS_EVT_CONN_INFO_NTF_ENABLE
@ THSCPS_EVT_CONN_INFO_NTF_ENABLE
THS Connection Information notification is enabled.
Definition: thscps.h:154
THSCPS_CODED_PHY
@ THSCPS_CODED_PHY
LE Coded PHY.
Definition: thscps.h:99
thscps_evt_type_t
thscps_evt_type_t
THS Control Point Service Event Type.
Definition: thscps.h:146
sdk_err_t
uint16_t sdk_err_t
SDK API result type.
Definition: ble_error.h:243
thscps_test_role_t
thscps_test_role_t
Local device GAP Role Type.
Definition: thscps.h:87
THSCPS_EVT_SETTING_SET
@ THSCPS_EVT_SETTING_SET
Throughput setting.
Definition: thscps.h:160
THSCPS_RSP_ID_UNSUPPORT
@ THSCPS_RSP_ID_UNSUPPORT
Failed because of unsupport command.
Definition: thscps.h:137
thscps_test_conn_info_t::ths_mode
uint8_t ths_mode
THS Mode.
Definition: thscps.h:194
thscps_adv_param_t::phy
thscps_adv_phy_t phy
Specify what PHY the Controller has changed for TX/RX.
Definition: thscps.h:200
thscps_test_conn_info_t::rx_phy
uint8_t rx_phy
RX PHY.
Definition: thscps.h:192
THSCPS_EVT_CTRL_PT_IND_DISABLE
@ THSCPS_EVT_CTRL_PT_IND_DISABLE
THS Control Point indicaiton is disabled.
Definition: thscps.h:149
THSCPS_RSP_ID_TEST_ROLE_ERR
@ THSCPS_RSP_ID_TEST_ROLE_ERR
Failed becaude of Test role error.
Definition: thscps.h:140
THSCPS_CTRL_PT_ADV_PARAM
@ THSCPS_CTRL_PT_ADV_PARAM
Advertising parameters set.
Definition: thscps.h:114
THSCPS_SETTINGS_TYPE_TRANS_MODE
@ THSCPS_SETTINGS_TYPE_TRANS_MODE
Data transmission mode.
Definition: thscps.h:128
thscps_test_conn_info_t::tx_phy
uint8_t tx_phy
TX PHY.
Definition: thscps.h:191
thscps_test_conn_info_t::tx_power
int8_t tx_power
TX Power.
Definition: thscps.h:193
thscps_rsp_val_t::conn_idx
uint8_t conn_idx
Connection of cmd set.
Definition: thscps.h:211
thscps_ctrl_pt_id_t
thscps_ctrl_pt_id_t
THS Control Point Service Control Point IDs.
Definition: thscps.h:111
THSCPS_EVT_TSET_SET_NTF_ENABLE
@ THSCPS_EVT_TSET_SET_NTF_ENABLE
THS Test Information notification is enabled.
Definition: thscps.h:150
THSCPS_CTRL_PT_INVALID
@ THSCPS_CTRL_PT_INVALID
Invalid cmd id.
Definition: thscps.h:112
thscps_evt_t::evt_type
thscps_evt_type_t evt_type
THS client event type.
Definition: thscps.h:218
THSCPS_TEST_STOP
@ THSCPS_TEST_STOP
Throughput Test is not ongoing.
Definition: thscps.h:105
thscps_evt_handler_t
void(* thscps_evt_handler_t)(thscps_evt_t *p_evt)
THS Control Point Service event handler type.
Definition: thscps.h:234
thscps_evt_t::conn_idx
uint8_t conn_idx
The connection index.
Definition: thscps.h:217
THSCPS_SETTINGS_TYPE_TOGGLE
@ THSCPS_SETTINGS_TYPE_TOGGLE
Throughput toggle state of sending the data.
Definition: thscps.h:130
THSCPS_SETTINGS_TYPE_MTU
@ THSCPS_SETTINGS_TYPE_MTU
MTU Size.
Definition: thscps.h:125
THSCPS_TEST_ROLE_SLAVE
@ THSCPS_TEST_ROLE_SLAVE
Test role: Slave.
Definition: thscps.h:89
thscps_test_conn_info_t::pdu
uint16_t pdu
PDU.
Definition: thscps.h:189
THSCPS_EVT_CONN_INFO_NTF_DISABLE
@ THSCPS_EVT_CONN_INFO_NTF_DISABLE
THS Connection Information notification is disabled.
Definition: thscps.h:155
THSCPS_CTRL_PT_ADV_ACTION
@ THSCPS_CTRL_PT_ADV_ACTION
Advertiding action.
Definition: thscps.h:115
thscps_rsp_val_t
THS Control Point Response value.
Definition: thscps.h:208
thscps_test_info_t::packets_val
uint16_t packets_val
Recieved Packects value.
Definition: thscps.h:182
THSCPS_EVT_INVALID
@ THSCPS_EVT_INVALID
Throughput Control Point Service invalid event.
Definition: thscps.h:147
thscps_rsp_val_t::cmd_id
uint8_t cmd_id
Commander ID.
Definition: thscps.h:209
THSCPS_EVT_ADV_ACTION
@ THSCPS_EVT_ADV_ACTION
Set advertising action.
Definition: thscps.h:158
THSCPS_TEST_ROLE_INVALID
@ THSCPS_TEST_ROLE_INVALID
Test role: Invalid.
Definition: thscps.h:88
THSCPS_TEST_STARTED
@ THSCPS_TEST_STARTED
Throughput Test is ongoing.
Definition: thscps.h:106