Public Attributes | List of all members
ble_escs_init_params_t Struct Reference
BLE Services » BLE Eddystone Configuration Service (ESCS)

EddyStone Configuration Service environment variable. More...

`#include <escs.h>`

Collaboration diagram for ble_escs_init_params_t:
[legend]

## Public Attributes
uint8_t | active_slot_no
| curret active slot number.
uint8_t | lock_state
| beacon lock state.
uint16_t | adv_interval
| advertising interval.
int8_t | slot_tx_power [APP_MAX_ADV_SLOTS]
| radio tx power.
int8_t | adv_tx_power
| advertised tx Power.
bool | remain_connectable
| whether to remain connectable.
slot_lock_code_t | beacon_lock_code
| beacon lock code.

## Detailed Description

EddyStone Configuration Service environment variable.

The documentation for this struct was generated from the following file:

- escs.h