Macros
Transfer Priority level
Peripheral Driver » LL Driver » DMA » Defines » DMA Exported Constants

## Macros
#define | LL_DMA_PRIORITY_0 DMA_CFGL_CH_PRIOR_0
#define | LL_DMA_PRIORITY_1 DMA_CFGL_CH_PRIOR_1
#define | LL_DMA_PRIORITY_2 DMA_CFGL_CH_PRIOR_2
#define | LL_DMA_PRIORITY_3 DMA_CFGL_CH_PRIOR_3
#define | LL_DMA_PRIORITY_4 DMA_CFGL_CH_PRIOR_4
#define | LL_DMA_PRIORITY_5 DMA_CFGL_CH_PRIOR_5
#define | LL_DMA_PRIORITY_6 DMA_CFGL_CH_PRIOR_6
#define | LL_DMA_PRIORITY_7 DMA_CFGL_CH_PRIOR_7

## Detailed Description

## Macro Definition Documentation

## ◆ LL_DMA_PRIORITY_0

#define LL_DMA_PRIORITY_0 DMA_CFGL_CH_PRIOR_0

Priority level : 0

## ◆ LL_DMA_PRIORITY_1

#define LL_DMA_PRIORITY_1 DMA_CFGL_CH_PRIOR_1

Priority level : 1

## ◆ LL_DMA_PRIORITY_2

#define LL_DMA_PRIORITY_2 DMA_CFGL_CH_PRIOR_2

Priority level : 2

## ◆ LL_DMA_PRIORITY_3

#define LL_DMA_PRIORITY_3 DMA_CFGL_CH_PRIOR_3

Priority level : 3

## ◆ LL_DMA_PRIORITY_4

#define LL_DMA_PRIORITY_4 DMA_CFGL_CH_PRIOR_4

Priority level : 4

## ◆ LL_DMA_PRIORITY_5

#define LL_DMA_PRIORITY_5 DMA_CFGL_CH_PRIOR_5

Priority level : 5

## ◆ LL_DMA_PRIORITY_6

#define LL_DMA_PRIORITY_6 DMA_CFGL_CH_PRIOR_6

Priority level : 6

## ◆ LL_DMA_PRIORITY_7

#define LL_DMA_PRIORITY_7 DMA_CFGL_CH_PRIOR_7

Priority level : 7