Macros
QSPI Address and Instruction Transfer Format
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SSI_INST_ADDR_ALL_IN_SPI 0x00000000UL
#define | LL_SSI_INST_IN_SPI_ADDR_IN_SPIFRF (1UL << SSI_SCTRL0_TRANSTYPE_Pos)
#define | LL_SSI_INST_ADDR_ALL_IN_SPIFRF (2UL << SSI_SCTRL0_TRANSTYPE_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SSI_INST_ADDR_ALL_IN_SPI

#define LL_SSI_INST_ADDR_ALL_IN_SPI 0x00000000UL

Instruction and address are sent in SPI mode

## ◆ LL_SSI_INST_ADDR_ALL_IN_SPIFRF

#define LL_SSI_INST_ADDR_ALL_IN_SPIFRF (2UL << SSI_SCTRL0_TRANSTYPE_Pos)

Instruction and address are sent in Daul/Quad SPI mode

## ◆ LL_SSI_INST_IN_SPI_ADDR_IN_SPIFRF

#define LL_SSI_INST_IN_SPI_ADDR_IN_SPIFRF (1UL << SSI_SCTRL0_TRANSTYPE_Pos)

Instruction is in sent in SPI mode and address is sent in Daul/Quad SPI mode