Data Fields
gap_adv_period_cfg_t Struct Reference
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Management » Structures

Configuration for periodic advertising. More...

`#include <ble_gapm.h>`

## Data Fields
uint16_t | adv_intv_min
uint16_t | adv_intv_max

## Detailed Description

Configuration for periodic advertising.

## Field Documentation

## ◆ adv_intv_max

uint16_t gap_adv_period_cfg_t::adv_intv_max

Maximum advertising interval (in unit of 1.25 ms). Must be greater than 20 ms.

## ◆ adv_intv_min

uint16_t gap_adv_period_cfg_t::adv_intv_min

Minimum advertising interval (in unit of 1.25 ms). Must be greater than 20 ms.

The documentation for this struct was generated from the following file:

- ble_gapm.h