Macros
Force Clock OFF
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

## Macros
#define | LL_CGC_FRC_AON_MCUSUB_HCLK MCU_SUB_FORCE_AON_MCUSUB_HCLK
#define | LL_CGC_FRC_XF_XQSPI_HCLK MCU_SUB_FORCE_XF_XQSPI_HCLK
#define | LL_CGC_FRC_SRAM_HCLK MCU_SUB_FORCE_SRAM_HCLK
#define | LL_CGC_FRC_ALL_HCLK1 ((uint32_t)0x00070000U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_FRC_ALL_HCLK1

#define LL_CGC_FRC_ALL_HCLK1 ((uint32_t)0x00070000U)

All clock group 1

## ◆ LL_CGC_FRC_AON_MCUSUB_HCLK

#define LL_CGC_FRC_AON_MCUSUB_HCLK MCU_SUB_FORCE_AON_MCUSUB_HCLK

Hclk for Always-on register

## ◆ LL_CGC_FRC_SRAM_HCLK

#define LL_CGC_FRC_SRAM_HCLK MCU_SUB_FORCE_SRAM_HCLK

Hclk for SRAMs

## ◆ LL_CGC_FRC_XF_XQSPI_HCLK

#define LL_CGC_FRC_XF_XQSPI_HCLK MCU_SUB_FORCE_XF_XQSPI_HCLK

Hclk for cache top