Data Fields
ans_init_t Struct Reference
BLE Services » Alert Notification Service (ANS) » Structures

Alert Notification Service init stucture. This contains all options and data needed for initialization of the service. More...

`#include <ans.h>`

## Data Fields
ans_evt_handler_t | evt_handler
uint16_t | sup_new_alert_cat
uint16_t | sup_unread_alert_sta

## Detailed Description

Alert Notification Service init stucture. This contains all options and data needed for initialization of the service.

## Field Documentation

## ◆ evt_handler

ans_evt_handler_t ans_init_t::evt_handler

Phone Alert Status Service event handler.

## ◆ sup_new_alert_cat

uint16_t ans_init_t::sup_new_alert_cat

Initial mask of Supported New Alert Category.

## ◆ sup_unread_alert_sta

uint16_t ans_init_t::sup_unread_alert_sta

Initial mask of Unread Alert Status.

The documentation for this struct was generated from the following file:

- ans.h