Macros
Resistor Enable
Peripheral Driver » LL Driver » GPIO » Defines » GPIO Private Macros

## Macros
#define | LL_GPIO_RE_N_Pos 0
#define | LL_GPIO_RE_N_Msk (0x1U << LL_GPIO_RE_N_Pos)
#define | LL_GPIO_RE_N LL_GPIO_RE_N_Msk

## Detailed Description

## Macro Definition Documentation

## ◆ LL_GPIO_RE_N

#define LL_GPIO_RE_N LL_GPIO_RE_N_Msk

Resistor Enable bits

## ◆ LL_GPIO_RE_N_Msk

#define LL_GPIO_RE_N_Msk (0x1U << LL_GPIO_RE_N_Pos)

Resistor Enable bits mask

## ◆ LL_GPIO_RE_N_Pos

#define LL_GPIO_RE_N_Pos 0

Resistor Enable bits position