Data Fields
hts_meas_val_t Struct Reference
BLE Services » Health Thermometer Service (HTS) » Structures

Health Theromometer Measurement Character value structure. More...

`#include <hts.h>`

## Data Fields
hts_temp_meas_type_t | temp_meas_type
uint16_t | temp_original_value
ieee_float32_t | temp_convert_value
hts_date_time_t | time_stamp
hts_temp_meas_loc_t | temp_type

## Detailed Description

Health Theromometer Measurement Character value structure.

## Field Documentation

## ◆ temp_convert_value

ieee_float32_t hts_meas_val_t::temp_convert_value

Temperature measurement convert value.

## ◆ temp_meas_type

hts_temp_meas_type_t hts_meas_val_t::temp_meas_type

Stable or intermediary type of temperature.

## ◆ temp_original_value

uint16_t hts_meas_val_t::temp_original_value

Temperature measurement original value.

## ◆ temp_type

hts_temp_meas_loc_t hts_meas_val_t::temp_type

Temperature Type measurement location.

## ◆ time_stamp

hts_date_time_t hts_meas_val_t::time_stamp

Time Stamp.

The documentation for this struct was generated from the following file:

- hts.h