Macros
IT Defines
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

Interrupt definitions which can be used with LL_SPI_ReadReg and LL_SPI_WriteReg functions. More...

## Macros
#define | LL_SSI_IM_MST SSI_INTMASK_MSTIM
#define | LL_SSI_IM_RXF SSI_INTMASK_RXFIM
#define | LL_SSI_IM_RXO SSI_INTMASK_RXOIM
#define | LL_SSI_IM_RXU SSI_INTMASK_RXUIM
#define | LL_SSI_IM_TXO SSI_INTMASK_TXOIM
#define | LL_SSI_IM_TXE SSI_INTMASK_TXEIM
#define | LL_SSI_IS_MST SSI_INTSTAT_MSTIS
#define | LL_SSI_IS_RXF SSI_INTSTAT_RXFIS
#define | LL_SSI_IS_RXO SSI_INTSTAT_RXOIS
#define | LL_SSI_IS_RXU SSI_INTSTAT_RXUIS
#define | LL_SSI_IS_TXO SSI_INTSTAT_TXOIS
#define | LL_SSI_IS_TXE SSI_INTSTAT_TXEIS
#define | LL_SSI_RIS_MST SSI_RAW_INTSTAT_MSTIR
#define | LL_SSI_RIS_RXF SSI_RAW_INTSTAT_RXFIR
#define | LL_SSI_RIS_RXO SSI_RAW_INTSTAT_RXOIR
#define | LL_SSI_RIS_RXU SSI_RAW_INTSTAT_RXUIR
#define | LL_SSI_RIS_TXO SSI_RAW_INTSTAT_TXOIR
#define | LL_SSI_RIS_TXE SSI_RAW_INTSTAT_TXEIR

## Detailed Description

Interrupt definitions which can be used with LL_SPI_ReadReg and LL_SPI_WriteReg functions.

## Macro Definition Documentation

## ◆ LL_SSI_IM_MST

#define LL_SSI_IM_MST SSI_INTMASK_MSTIM

Multi-Master Contention Interrupt enable

## ◆ LL_SSI_IM_RXF

#define LL_SSI_IM_RXF SSI_INTMASK_RXFIM

Receive FIFO Full Interrupt enable

## ◆ LL_SSI_IM_RXO

#define LL_SSI_IM_RXO SSI_INTMASK_RXOIM

Receive FIFO Overflow Interrupt enable

## ◆ LL_SSI_IM_RXU

#define LL_SSI_IM_RXU SSI_INTMASK_RXUIM

Receive FIFO Underflow Interrupt enable

## ◆ LL_SSI_IM_TXE

#define LL_SSI_IM_TXE SSI_INTMASK_TXEIM

Transmit FIFO Empty Interrupt enable

## ◆ LL_SSI_IM_TXO

#define LL_SSI_IM_TXO SSI_INTMASK_TXOIM

Transmit FIFO Overflow Interrupt enable

## ◆ LL_SSI_IS_MST

#define LL_SSI_IS_MST SSI_INTSTAT_MSTIS

Multi-Master Contention Interrupt flag

## ◆ LL_SSI_IS_RXF

#define LL_SSI_IS_RXF SSI_INTSTAT_RXFIS

Receive FIFO Full Interrupt flag

## ◆ LL_SSI_IS_RXO

#define LL_SSI_IS_RXO SSI_INTSTAT_RXOIS

Receive FIFO Overflow Interrupt flag

## ◆ LL_SSI_IS_RXU

#define LL_SSI_IS_RXU SSI_INTSTAT_RXUIS

Receive FIFO Underflow Interrupt flag

## ◆ LL_SSI_IS_TXE

#define LL_SSI_IS_TXE SSI_INTSTAT_TXEIS

Transmit FIFO Empty Interrupt flag

## ◆ LL_SSI_IS_TXO

#define LL_SSI_IS_TXO SSI_INTSTAT_TXOIS

Transmit FIFO Overflow Interrupt flag

## ◆ LL_SSI_RIS_MST

#define LL_SSI_RIS_MST SSI_RAW_INTSTAT_MSTIR

Multi-Master Contention RAW Interrupt flag

## ◆ LL_SSI_RIS_RXF

#define LL_SSI_RIS_RXF SSI_RAW_INTSTAT_RXFIR

Receive FIFO Full RAW Interrupt flag

## ◆ LL_SSI_RIS_RXO

#define LL_SSI_RIS_RXO SSI_RAW_INTSTAT_RXOIR

Receive FIFO Overflow RAW Interrupt flag

## ◆ LL_SSI_RIS_RXU

#define LL_SSI_RIS_RXU SSI_RAW_INTSTAT_RXUIR

Receive FIFO Underflow RAW Interrupt flag

## ◆ LL_SSI_RIS_TXE

#define LL_SSI_RIS_TXE SSI_RAW_INTSTAT_TXEIR

Transmit FIFO Empty RAW Interrupt flag

## ◆ LL_SSI_RIS_TXO

#define LL_SSI_RIS_TXO SSI_RAW_INTSTAT_TXOIR

Transmit FIFO Overflow RAW Interrupt flag