Macros
MicroWire Control
Peripheral Driver » LL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | LL_SSI_MICROWIRE_HANDSHAKE_DIS 0x00000000UL
#define | LL_SSI_MICROWIRE_HANDSHAKE_EN (1UL << SSI_MWC_MHS_Pos)
#define | LL_SSI_MICROWIRE_RX 0x00000000UL
#define | LL_SSI_MICROWIRE_TX (1UL << SSI_MWC_MDD_Pos)
#define | LL_SSI_MICROWIRE_NON_SEQUENTIAL 0x00000000UL
#define | LL_SSI_MICROWIRE_SEQUENTIAL (1UL << SSI_MWC_MWMOD_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_SSI_MICROWIRE_HANDSHAKE_DIS

#define LL_SSI_MICROWIRE_HANDSHAKE_DIS 0x00000000UL

Enable Handshake for Microwire transfer

## ◆ LL_SSI_MICROWIRE_HANDSHAKE_EN

#define LL_SSI_MICROWIRE_HANDSHAKE_EN (1UL << SSI_MWC_MHS_Pos)

Disable Handshake for Microwire transfer

## ◆ LL_SSI_MICROWIRE_NON_SEQUENTIAL

#define LL_SSI_MICROWIRE_NON_SEQUENTIAL 0x00000000UL

Non-sequential for Microwire transfer

## ◆ LL_SSI_MICROWIRE_RX

#define LL_SSI_MICROWIRE_RX 0x00000000UL

Rx mode. Rx transfer at Microwire mode

## ◆ LL_SSI_MICROWIRE_SEQUENTIAL

#define LL_SSI_MICROWIRE_SEQUENTIAL (1UL << SSI_MWC_MWMOD_Pos)

Sequential for Microwire transfer

## ◆ LL_SSI_MICROWIRE_TX

#define LL_SSI_MICROWIRE_TX (1UL << SSI_MWC_MDD_Pos)

Tx mode. Tx transfer at Microwire mode