Macros
Defines
Peripheral Driver » APP DRIVER » DRIVER CONFIG

## Macros
#define | APP_DRIVER_ADC_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
| APP driver peripheral priority define. More...
#define | APP_DRIVER_AES_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
#define | APP_DRIVER_COMP_WAPEUP_PRIORITY WAPEUP_PRIORITY_LOW
#define | APP_DRIVER_DUAL_TIM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
#define | APP_DRIVER_DMA_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
#define | APP_DRIVER_GPIOTE_WAPEUP_PRIORITY WAPEUP_PRIORITY_LOW
#define | APP_DRIVER_SYSTICK_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
#define | APP_DRIVER_UART_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
#define | APP_DRIVER_HMAC_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
#define | APP_DRIVER_I2C_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
#define | APP_DRIVER_I2S_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
#define | APP_DRIVER_QSPI_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
#define | APP_DRIVER_RNG_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
#define | APP_DRIVER_SPI_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH
#define | APP_DRIVER_TIM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID
#define | APP_DRIVER_PWM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

## Detailed Description

## Macro Definition Documentation

## ◆ APP_DRIVER_ADC_WAPEUP_PRIORITY

#define APP_DRIVER_ADC_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

APP driver peripheral priority define.

ADC Wakeup priority High

## ◆ APP_DRIVER_AES_WAPEUP_PRIORITY

#define APP_DRIVER_AES_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

AES Wakeup priority Mid

## ◆ APP_DRIVER_COMP_WAPEUP_PRIORITY

#define APP_DRIVER_COMP_WAPEUP_PRIORITY WAPEUP_PRIORITY_LOW

COMP Wakeup priority Low

## ◆ APP_DRIVER_DMA_WAPEUP_PRIORITY

#define APP_DRIVER_DMA_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

DMA Wakeup priority High

## ◆ APP_DRIVER_DUAL_TIM_WAPEUP_PRIORITY

#define APP_DRIVER_DUAL_TIM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

DUAL TIM Wakeup priority Mid

## ◆ APP_DRIVER_GPIOTE_WAPEUP_PRIORITY

#define APP_DRIVER_GPIOTE_WAPEUP_PRIORITY WAPEUP_PRIORITY_LOW

GPIOTE Wakeup priority Low

## ◆ APP_DRIVER_HMAC_WAPEUP_PRIORITY

#define APP_DRIVER_HMAC_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

Hmac Wakeup priority Mid

## ◆ APP_DRIVER_I2C_WAPEUP_PRIORITY

#define APP_DRIVER_I2C_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

I2C Wakeup priority High

## ◆ APP_DRIVER_I2S_WAPEUP_PRIORITY

#define APP_DRIVER_I2S_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

I2S Wakeup priority High

## ◆ APP_DRIVER_PWM_WAPEUP_PRIORITY

#define APP_DRIVER_PWM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

PWM Wakeup priority Mid

## ◆ APP_DRIVER_QSPI_WAPEUP_PRIORITY

#define APP_DRIVER_QSPI_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

QSPI Wakeup priority High

## ◆ APP_DRIVER_RNG_WAPEUP_PRIORITY

#define APP_DRIVER_RNG_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

RNG Wakeup priority Mid

## ◆ APP_DRIVER_SPI_WAPEUP_PRIORITY

#define APP_DRIVER_SPI_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

SPI Wakeup priority High

## ◆ APP_DRIVER_SYSTICK_WAPEUP_PRIORITY

#define APP_DRIVER_SYSTICK_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

SysTick Wakeup priority High

## ◆ APP_DRIVER_TIM_WAPEUP_PRIORITY

#define APP_DRIVER_TIM_WAPEUP_PRIORITY WAPEUP_PRIORITY_MID

TIM Wakeup priority Mid

## ◆ APP_DRIVER_UART_WAPEUP_PRIORITY

#define APP_DRIVER_UART_WAPEUP_PRIORITY WAPEUP_PRIORITY_HIGH

Uart Wakeup priority High