Macros
Block2 Clock During WFI
Peripheral Driver » LL Driver » CGC » Defines » CGC Exported Constants

## Macros
#define | LL_CGC_WFI_SECU_DIV4_PCLK MCU_SUB_WFI_SECU_DIV4_PCLK
#define | LL_CGC_WFI_XQSPI_DIV4_PCLK MCU_SUB_WFI_XQSPI_DIV4_PCLK
#define | LL_CGC_WFI_ALL_HCLK2 ((uint32_t)0x05000000U)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_CGC_WFI_ALL_HCLK2

#define LL_CGC_WFI_ALL_HCLK2 ((uint32_t)0x05000000U)

All clock group 2

## ◆ LL_CGC_WFI_SECU_DIV4_PCLK

#define LL_CGC_WFI_SECU_DIV4_PCLK MCU_SUB_WFI_SECU_DIV4_PCLK

Div4 clk for security blocks

## ◆ LL_CGC_WFI_XQSPI_DIV4_PCLK

#define LL_CGC_WFI_XQSPI_DIV4_PCLK MCU_SUB_WFI_XQSPI_DIV4_PCLK

Div4 clk for xf qspi