Data Fields
_pkc_rsa_modular_exponent Struct Reference
Peripheral Driver » HAL Driver » PKC » Structures » PKC expression input

PKC RSA Modular Exponentiation expression input. More...

`#include <gr55xx_hal_pkc.h>`

## Data Fields
uint32_t * | p_A
uint32_t * | p_B
uint32_t * | p_P
uint32_t * | p_P_R2
uint32_t | ConstP

## Detailed Description

PKC RSA Modular Exponentiation expression input.

Note
  Result = A^B mod P

## Field Documentation

## ◆ ConstP

uint32_t _pkc_rsa_modular_exponent::ConstP

Montgomery multiplication constant of P

## ◆ p_A

uint32_t* _pkc_rsa_modular_exponent::p_A

Pointer to operand A

## ◆ p_B

uint32_t* _pkc_rsa_modular_exponent::p_B

Pointer to operand B

## ◆ p_P

uint32_t* _pkc_rsa_modular_exponent::p_P

Pointer to prime number P

## ◆ p_P_R2

uint32_t* _pkc_rsa_modular_exponent::p_P_R2

P_R2 = R^2 mod P, where R = 2^DataBits

The documentation for this struct was generated from the following file:

- gr55xx_hal_pkc.h