Enumerations
Enumerations
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control

## Enumerations
enum | gap_get_conn_info_op_t { GAP_GET_CON_RSSI = 0, GAP_GET_CON_CHANNEL_MAP, GAP_GET_PHY, GAP_GET_CHAN_SEL_ALGO }
| The operation code used to get connection info. More...
enum | gap_get_peer_info_op_t { GAP_GET_PEER_VERSION = 0, GAP_GET_PEER_FEATURES }
| The operation code used to get peer device info. More...
enum | gap_adv_report_type_t { GAP_REPORT_TYPE_ADV_EXT = 0, GAP_REPORT_TYPE_ADV_LEG, GAP_REPORT_TYPE_SCAN_RSP_EXT, GAP_REPORT_TYPE_SCAN_RSP_LEG, GAP_REPORT_TYPE_PER_ADV }
| Advertising report type. More...
enum | gap_adv_report_info_t { GAP_REPORT_INFO_COMPLETE_BIT = (1 << 0), GAP_REPORT_INFO_CONN_ADV_BIT = (1 << 1), GAP_REPORT_INFO_SCAN_ADV_BIT = (1 << 2), GAP_REPORT_INFO_DIR_ADV_BIT = (1 << 3) }
| Advertising report information. More...
enum | gap_stopped_reason_t { GAP_STOPPED_REASON_TIMEOUT = 0, GAP_STOPPED_REASON_ON_USER, GAP_STOPPED_REASON_CONN_EST }
| Stop reason code. More...
enum | gap_ll_role_type_t { GAP_LL_ROLE_MASTER = 0, GAP_LL_ROLE_SLAVE = 1 }
| Device role of LL layer type. More...
enum | gap_param_set_op_id_t { GAP_OPCODE_CHNL_MAP_SET, GAP_OPCODE_WHITELIST_SET, GAP_OPCODE_PER_ADV_LIST_SET, GAP_OPCODE_PRIVACY_MODE_SET }
| Operation code used to set param(s). More...
enum | gap_rslv_addr_read_op_id_t { GAP_OPCODE_LOCAL_RSLV_ADDR_READ, GAP_OPCODE_PEER_RSLV_ADDR_READ }
| Operation code used to read resolvable address. More...
enum | gap_psm_manager_op_id_t { GAP_OPCODE_LEPSM_REGISTER, GAP_OPCODE_LEPSM_UNREGISTER }
| Operation code used for LEPSM manager. More...
enum | gap_disconn_reason_t { GAP_HCI_AUTHENTICATION_FAILURE = 0x05, GAP_HCI_REMOTE_USER_TERMINATED_CONNECTION = 0x13, GAP_HCI_REMOTE_DEV_TERMINATION_DUE_TO_LOW_RESOURCES = 0x14, GAP_HCI_REMOTE_DEV_TERMINATION_DUE_TO_POWER_OFF = 0x15, GAP_HCI_UNSUPPORTED_REMOTE_FEATURE = 0x1A, GAP_HCI_PAIRING_WITH_UNIT_KEY_UNSUPPORTED = 0X29, GAP_HCI_CONN_INTERVAL_UNACCEPTABLE = 0x3B }
| The specified reason for terminating a connection. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ gap_adv_report_info_t

enum gap_adv_report_info_t

Advertising report information.

Enumerator
GAP_REPORT_INFO_COMPLETE_BIT | Report is complete.
GAP_REPORT_INFO_CONN_ADV_BIT | Connectable advertising.
GAP_REPORT_INFO_SCAN_ADV_BIT | Scannable advertising.
GAP_REPORT_INFO_DIR_ADV_BIT | Directed advertising.

## ◆ gap_adv_report_type_t

enum gap_adv_report_type_t

Advertising report type.

Enumerator
GAP_REPORT_TYPE_ADV_EXT | Extended advertising report.
GAP_REPORT_TYPE_ADV_LEG | Legacy advertising report.
GAP_REPORT_TYPE_SCAN_RSP_EXT | Extended scan response report.
GAP_REPORT_TYPE_SCAN_RSP_LEG | Legacy scan response report.
GAP_REPORT_TYPE_PER_ADV | Periodic advertising report.

## ◆ gap_disconn_reason_t

enum gap_disconn_reason_t

The specified reason for terminating a connection.

Enumerator
GAP_HCI_AUTHENTICATION_FAILURE | Authentication Failure.
GAP_HCI_REMOTE_USER_TERMINATED_CONNECTION | Remote User Terminated Connection.
GAP_HCI_REMOTE_DEV_TERMINATION_DUE_TO_LOW_RESOURCES | Remote Device Terminated Connection due to Low Resources .
GAP_HCI_REMOTE_DEV_TERMINATION_DUE_TO_POWER_OFF | Remote Device Terminated Connection due to Power Off.
GAP_HCI_UNSUPPORTED_REMOTE_FEATURE | Unsupported Remote Feature.
GAP_HCI_PAIRING_WITH_UNIT_KEY_UNSUPPORTED | Pairing With Unit Key Not Supported.
GAP_HCI_CONN_INTERVAL_UNACCEPTABLE | Unacceptable Connection Parameters.

## ◆ gap_get_conn_info_op_t

enum gap_get_conn_info_op_t

The operation code used to get connection info.

Enumerator
GAP_GET_CON_RSSI | Get connection RSSI info.
GAP_GET_CON_CHANNEL_MAP | Get connection channel map.
GAP_GET_PHY | Get connection PHY.
GAP_GET_CHAN_SEL_ALGO | Get selection algorithm for connection channel.

## ◆ gap_get_peer_info_op_t

enum gap_get_peer_info_op_t

The operation code used to get peer device info.

Enumerator
GAP_GET_PEER_VERSION | Get peer device version info.
GAP_GET_PEER_FEATURES | Get peer device features info.

## ◆ gap_ll_role_type_t

enum gap_ll_role_type_t

Device role of LL layer type.

Enumerator
GAP_LL_ROLE_MASTER | Master role.
GAP_LL_ROLE_SLAVE | Slave role.

## ◆ gap_param_set_op_id_t

enum gap_param_set_op_id_t

Operation code used to set param(s).

Enumerator
GAP_OPCODE_CHNL_MAP_SET | Set Channel Map.
GAP_OPCODE_WHITELIST_SET | Set white list.
GAP_OPCODE_PER_ADV_LIST_SET | Set periodic advertising list.
GAP_OPCODE_PRIVACY_MODE_SET | Set privacy mode for peer device.

## ◆ gap_psm_manager_op_id_t

enum gap_psm_manager_op_id_t

Operation code used for LEPSM manager.

Enumerator
GAP_OPCODE_LEPSM_REGISTER | LEPSM register operation.
GAP_OPCODE_LEPSM_UNREGISTER | LEPSM unregister operation.

## ◆ gap_rslv_addr_read_op_id_t

enum gap_rslv_addr_read_op_id_t

Operation code used to read resolvable address.

Enumerator
GAP_OPCODE_LOCAL_RSLV_ADDR_READ | Local resolvable address operation.
GAP_OPCODE_PEER_RSLV_ADDR_READ | Peer resolvable address operation.

## ◆ gap_stopped_reason_t

enum gap_stopped_reason_t

Stop reason code.

Enumerator
GAP_STOPPED_REASON_TIMEOUT | Stop with timeout.
GAP_STOPPED_REASON_ON_USER | Stop with user stopping it actively.
GAP_STOPPED_REASON_CONN_EST | Stop with connection established.